For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement in Lighting Systems.
3. Remove the screw from the vehicle inside.
4. Remove the roof antenna.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the roof antenna with the screw.

Tighten
Tighten the roof antenna retaining screws to 3 N·m (27 lb in).

2. Install the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement in Lighting Systems.
3. Connect the negative battery cable.