For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the CMP sensor connectors.
3. Remove the CMP sensor bolt (2).
4. Remove the CMP sensor (1).

### Installation Procedure

1. Install the CMP sensor (1).
2. Install the CMP sensor bolt (2).
3. Connect the CMP sensor connectors.
4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.