For 1990-2009 cars

Important: Apply putty in areas indicated before painting.

#### Engine Room - 1 of 2

(1) | Spot Weld Sealer
(2) | Body Sealer
(3) | Dash Upper Cross Member
(4) | Spot Tape Seal
(5) | Dash Upper Bulkhead
(6) | Dash Upper Panel
(7) | Dash Panel
(8) | Dash Center Cross Member
(9) | Wheelhouse Extension
(10) | Wheelhouse Rear Panel
(11) | Front Outer Longitudinal
(12) | Front Inner Longitudinal

Important: Apply putty in areas indicated before painting.

#### Engine Room - 2 of 2

(1) | Spot Weld Sealer
(2) | Body Sealer
(3) | Sealant to be wiped
(4) | Dash Top Panel
(5) | Side Outer Panel
(6) | Front Pillar Lower Reinforcement
(7) | Sealing area
(8) | Hood Hinge Lower Bracket
(9) | Dash Side Panel

Important: Apply putty in areas indicated before painting.

#### Dash

(1) | Spot Tape Seal

Important: Apply putty in areas indicated before painting.

#### Floor and Rear Compartment

(1) | Body Sealer
(2) | Caulking Sealer

#### Rear Lamp and Rear Compartment

(1) | Side Inner Panel
(2) | Side Outer Panel
(3) | Body Sealer
(4) | Tail Lamp Housing
(5) | Back Lower Side Reinforcement
(6) | Lamp Housing Lower
(7) | Side Inner Panel
(8) | Back Lower Panel

#### Rear Lamp and Rear Compartment - Notchback

(1) | Body Sealer
(2) | Side Outer Panel
(3) | Fuel Filler Cap

Important: Keep roof mounting clips free of sealant on both side of roof.

Wipe off excess sealant from screen flange.

#### Roof - 1 of 2

(1) | Side Outer Panel
(2) | Body Sealer
(3) | Roof Panel
(4) | Roof Side Inner Panel
(5) | Front Pillar Upper Reinforcement
(6) | Sealer to be Wiped for Roof Molding Mounting
(7) | Sealer to be Wiped for Glass Matching

#### Roof - 2 of 2

(1) | Adhesive
(2) | Roof Panel
(3) | Roof Center Support

#### Sunroof

(1) | Adhesive
(2) | Roof Panel
(3) | Sunroof Frame
(4) | Windshield Header Rail
(5) | Roof Inner Rear Frame

Important: Paint drain holes in order to be free of sealer.

#### Hood

(1) | Sealer to be Wiped in this Area
(2) | Body Sealer

Important: Paint drain holes in order to be free of sealer.

#### Rear Compartment Lid

(1) | Area to be Closed by Sealer
(2) | Body Sealer
(3) | Water Drain Hole to be Free of Sealer

Important: Ensure water drain holes are free of sealer in the 5 locations on both doors.

#### Front and Rear Door

(1) | Water Drain Holes to be Free of Sealer
(2) | Sealer to be Wiped Around Door Corners
(3) | Apply Wax to Door Hinge