For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable.
2. Remove the screws (6, 7, 8) and the lower steering column cover panel (5).
3. Remove the ignition switch screw (1).
4. Remove the ignition switch (2).
5. Disconnect the ignition switch connector.

### Installation Procedure

1. Install the ignition switch (2) and the screw (1).
2. Connect the ignition switch connector.
3. Install the lower steering column cover panel (5) and the screws (6, 7, 8).
4. Connect the negative battery cable.