For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Mounting Bracket Bolts | 38 N·m | 28 lb ft
Adjusting Bolt | 22 N·m | 16 lb ft
Air Cleaner Housing Nuts | 12 N·m | 106 lb in
Camshaft Gear Bolt | 55 N·m | 41 lb ft
Camshaft Thrust Plate Screws | 10 N·m | 89 lb in
Catalytic Converter Lower Flange Nuts | 40 N·m | 30 lb ft
Catalytic Converter to Exhaust Manifold Nuts | 25-35 N·m | 18-25 lb ft
Connecting Rod Bearing Cap Nuts | 33 N·m | 24 lb ft
Crankshaft Main Bearing Cap Bolts | 57 N·m | 42 lb ft
Crankshaft Pulley Bolt | 70 N·m | 52 lb ft
Cylinder Head Bolts | 65-70 N·m | 48-52 lb ft
Cylinder Head Cover Hexagon Bolts | 9-12 N·m | 80-106 lb in
Engine Mount Brace Bracket Nuts | 20 N·m | 15 lb ft
Engine Mount Damping Block Bolts | 50 N·m | 37 lb ft
Engine Mount Intermediate Bracket Bolts | 55 N·m | 41 lb ft
Engine Mount Intermediate Bracket Upper Nuts | 65 N·m | 44 lb ft
Engine Mount Lower Bracket Bolts | 38 N·m | 28 lb ft
Engine Mount Upper Bracket Bolts | 38 N·m | 28 lb ft
Exhaust Manifold Bolts/Nuts | 22 N·m | 16 lb ft
Exhaust Manifold Heat Shield Bolts | 10 N·m | 89 lb in
Flywheel Inspection Lower Bolts | 5.5 N·m | 49 lb in
Front Exhaust Pipe Bracket Bolts | 40 N·m | 30 lb ft
Front Exhaust Pipe Nuts | 30 N·m | 22 lb ft
Generator Belt Tension Adjusting Bolt | 23 N·m | 17 lb ft
Generator Lower Bolts/Nut | 23 N·m | 17 lb ft
Generator Shackle Bolts | 30 N·m | 22 lb ft
Intake Manifold Main Bracket Bolts - 10M | 10 N·m | 89 lb in
Intake Manifold Main Bracket Nuts | 10 N·m | 89 lb in
Intake Manifold Nuts | 17 N·m | 13 lb ft
Intake Manifold Subsidiary Bracket Bolt | 10 N·m | 89 lb in
Intake Manifold Subsidiary Bracket Nut | 17 N·m | 13 lb ft
Intermediate Bracket Bolt | 55 N·m | 37 lb ft
Oil Level Gage Guide Tube Bolt | 10.5 N·m | 93 lb in
Oil Pan Bolts/Nuts | 10 N·m | 89 lb in
Oil Pump Cover Bolts | 10.5 N·m | 93 lb in
Oil Pump Pickup Tube Bolts | 10 N·m | 89 lb in
Oil Pump Strainer Bolt | 10.5 N·m | 93 lb in
Power Steering Rear Bracket Nut | 22 N·m | 16 lb ft
Rocker Arm Shaft Bolts | 10 N·m | 89 lb in
Timing Belt Front Lower Cover Bolts | 10.5 N·m | 93 lb in
Timing Belt Front Upper Cover Bolts | 10.5 N·m | 93 lb in
Timing Belt Rear Cover Bolts | 10.5 N·m | 93 lb in
Timing Belt Tensioner Bolt | 19 N·m | 14 lb ft
Valve Adjusting Lock Nuts | 17 N·m | 13 lb ft
Valve Cover Bolts | 10.5 N·m | 93 lb in
Water Outlet Case Nuts/Bolt | 10.5 N·m | 93 lb in