For 1990-2009 cars

## Starter Replacement 1.4L/1.5L SOHC and 1.4L/1.6L DOHC

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the upper and the lower starter mounting bolts.
3. Remove the starter solenoid nuts to disconnect the electrical cable.
4. Remove the starter assembly.

### Installation Procedure

1. Place the starter assembly in position.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the upper and the lower starter mounting bolts.

Tighten
Tighten the starter mounting bolts to 43 N·m (32 lb ft).

3. Position the starter electrical wire on the solenoid terminal.
4. Install the starter solenoid nuts.

Tighten
Tighten the starter solenoid nuts to 15 N·m (11 lb ft).

5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .

## Starter Replacement 1.2L SOHC

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector and clip around the starter.
3. Remove the engine oil temperature harness connector (2).
4. Remove the starter solenoid nut to disconnect the electrical cable (1).
5. Remove the harness clip bolt to disconnect the harness clip (4).
6. Remove the ground bolt (3).
7. Remove the starter mounting bolts (1).
8. Remove the starter assembly (2) from the engine.

### Installation Procedure

1. Install the starter to the engine.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the starter mounting bolts and starter solenoid nut.

Tighten

• | Tighten the starter mounting bolts to 23 N·m (17 lb ft).

• | Tighten the starter solenoid nut to 15 N·m (11 lb ft).

3. Install the ground bolt (3).

Tighten
Tighten the ground bolt to 41 N·m (30 lb ft).

4. Install the harness clip bolt (4).

Tighten
Tighten the harness clip bolt to 12 N·m (106 lb in).

5. Connect the engine oil temperature sensor connector (2).
6. Connect the negative battery cable.