For 1990-2009 cars

## Quarter Upper Trim Panel Replacement Notchback

### Removal Procedure

1. Remove the seat belt from the rear quarter upper trim panel.
2. Remove the rear quarter upper trim panel.

### Installation Procedure

1. Install the rear quarter upper trim panel.
2. Install the seat belt from the rear quarter upper trim panel.

## Quarter Upper Trim Panel Replacement 5 Door Hatchback

### Removal Procedure

1. Remove the seat belt from the rear quarter upper trim panel.
2. Remove the rear rocker trim panel.

Refer to Rear Side Door Sill Plate Replacement

3. Remove the rear quarter upper trim panel.

### Installation Procedure

1. Install the rear quarter upper trim panel.
2. Install the rear rocker trim panel.

Refer to Rear Side Door Sill Plate Replacement .

3. Install the seat belt from the rear quarter upper trim panel.

## Quarter Upper Trim Panel Replacement 3 Door Hatckback

### Removal Procedure

1. Remove the rear quarter trim panel. Refer to Rear Quarter Trim Panel Replacement.
2. Remove the seat belt upper anchor bolt (3).
3. Remove the two screws (3) from the rear compartment side cover (4).
4. Remove the rear compartment side cover (4).
5. Remove the upper quarter trim panel (1) from the vehicle.

### Installation Procedure

1. Install the upper quarter trim panel (1) to the vehicle.
2. Install the rear compartment side cover (4).
3. Install the two screws (3) to the rear compartment side cover (4).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the seat belt upper anchor bolt (3).

Tighten
Tighten the seat belt upper anchor bolt (3) to 38 N·m (28 lb ft).

5. Remove the rear quarter trim panel. Refer to Rear Quarter Trim Panel Replacement.