For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glove box. Refer to Instrument Panel Storage Compartment Replacement
3. Disconnect the passenger air bag disable switch connector.
4. Remove the passenger air bag disable switch by pushing the tab on the upper side of the switch housing.

### Installation Procedure

1. Install the passenger air bag disable switch.
2. Connect the passenger air bag disable switch connector.
3. Connect the negative battery cable.