For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
3. Disconnect the EVAP canister purge solenoid connector (2).
4. Disconnect the EVAP canister purge solenoid inlet and outlet hose.
5. Remove the EVAP canister purge solenoid (1) from the bracket.

### Installation Procedure

1. Install the EVAP canister purge solenoid (1) to the bracket.
2. Connect the EVAP canister purge solenoid inlet and outlet hose.
3. Connect the EVAP canister purge solenoid connector (2).
4. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.
5. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.