For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the camshaft position actuator valve connectors.
3. Remove the camshaft position actuator valve bolt.
4. Remove the camshaft position actuator valve (1) and seal.

### Installation Procedure

1. Install the camshaft position actuator valve (1) and seal. Coat seal with clean engine oil prior to installation.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the camshaft position actuator valve bolt.

Tighten
Tighten the camshaft position actuator valve bolt to 6 N·m (53 lb in).

3. Connect the camshaft position actuator valve connectors.
4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.