For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel center upper cover. Refer to Instrument Panel Center Trim Panel Replacement .
3. Remove the screws and the clock.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the clock with the screws.

Tighten
Tighten the clock screws to 2.5 N·m (23 lb in).

2. Install the instrument panel center upper cover. Refer to Instrument Panel Center Trim Panel Replacement .
3. Connect the negative battery cable.