For 1990-2009 cars

## Radio Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the instrument panel (I/P) lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement.
3. Remove the screws (1) and the audio system (2).
4. Disconnect the audio system electrical connector and the antenna cable.

### Installation Procedure

1. Connect the audio system electrical connector and the antenna cable.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the audio system (2) with the screws (1) and tighten to 6 N·m (53 lb in).
3. Install the I/P lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement.
4. Connect the negative battery cable.