For 1990-2009 cars

### Removal Procedure

1. Remove the upper center pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
2. Remove the bolts (2) and the seat belt height adjuster (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt height adjuster (1) with the bolts (2).

Tighten
Tighten the seat belt height adjuster bolts to 27 N·m (20 lb ft).

2. Install the upper center pillar trim panel. Refer to Center Pillar Upper Trim Panel Replacement .