For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the starter. Refer to Starter Motor Replacement.
3. Remove the CKP sensor bolt (1).
4. Remove the CKP sensor (2).

### Installation Procedure

1. Install the CKP sensor (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the CKP sensor bolt (1).

Tighten
Tighten the CKP sensor bolt (1) to 4.5 N·m (39.8 lb in).

3. Install the starter. Refer to Starter Motor Replacement.
4. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.