For 1990-2009 cars

## Front Seat Adjuster Replacement Horizontal

### Removal Procedure

1. Remove the seat back. Refer to Front Seat Back Replacement .
2. Remove the seat cushion bolts and the front seat adjusters from the seat cushion.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front seat adjusters to the seat cushion with the bolts.

Tighten
Tighten the front seat cushion bolts to 25 N·m (18 lb ft).

2. Install the seat back. Refer to Front Seat Back Replacement .