For 1990-2009 cars

## Rear Spoiler Replacement Hatchback

### Removal Procedure

1. Open the tail gate.
2. Remove the rear spoiler from the tail gate.

### Installation Procedure

Install the rear spoiler on the tail gate with the nuts.

## Rear Spoiler Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the clips and rear compartment trim.
3. Disconnect the rear spoiler electrical connector.
4. Remove the nuts.
5. Using a flat-bladed tool, carefully separate the rear spoiler from the rear compartment lid.
6. Remove the rear spoiler from the rear compartment lid.

### Installation Proccedure

Note: If reusing the rear spoiler, remove any remaining double-sided tape from the rear spoiler and the rear compartment lid.

1. Apply new double-sided tape.
2. Peel off the adhesive backing paper and affix the rear spoiler on to the rear compartment lid, ensuring it is carefully positioned.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the nuts attaching the rear spoiler and tighten to 3 N·m (27 lb in).
4. Install the rear compartment lid trim with the clips.
5. Connect the negative battery cable.