For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Disconnect the accelerator pedal position sensor connector.
3. Remove the 3 accelerator pedal retaining nuts (1).
4. Remove the accelerator pedal (2).

### Installation Procedure

1. Install the accelerator pedal (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 3 accelerator pedal retaining nuts (1).

Tighten
Tighten the accelerator pedal retaining nuts to 19 N·m (14 lb ft).

3. Connect the accelerator pedal position sensor connector.
4. Connect the battery cable. Refer to Battery Negative Cable Disconnection and Connection.