For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Nuts | 4.5 N·m | 40 lb in
Battery Carrier Tray Lower Bolts | 20 N·m | 15 lb ft
Battery Carrier Tray Upper Bolts | 20 N·m | 15 lb in
Battery Retainer Clamp-to-Battery Rod Nuts | 4 N·m | 35 lb in
Engine Mount Lower Bracket Bolts (1.2L) | 41 N·m | 30 lb ft
Front Bearing Plate Screws | 8 N·m | 71 lb in
Fuel Rail Retaining Bolts | 20 N·m | 15 lb in
Generator Adjusting Bolt (1.2L) | 7 N·m | 62 lb ft
Generator Battery Lead Nut | 15 N·m | 11 lb ft
Generator Brush Holder Screws | 12 N·m | 106 lb in
Generator Drive and End Bearing Nut | 81 N·m | 60 lb ft
Generator Drive End Bearing Nut | 81 N·m | 60 lb ft
Generator Lower Bracket Mounting Bolt (1.2L) | 28 N·m | 21 lb ft
Generator Lower Bracket-to-Generator Nuts | 25 N·m | 18 lb ft
Generator Pulley Nut (1.2L) | 110 N·m | 81 lb ft
Generator Shackle Bracket Bolt | 25 N·m | 18 lb ft
Generator Through-Bolts | 10 N·m | 89 lb in
Harness Ground Bolt | 41 N·m | 30 lb ft
Reaction Rod Bolt and Nut (1.2L) | 83 N·m | 61 lb ft
Starter Field Coil Connector Nut | 8 N·m | 71 lb in
Starter Mounting Bolts (1.2L) | 23 N·m | 17 lb ft
Starter Mounting Bolts (1.4L/1.5L SOHC and 1.4L/1.6L DOHC) | 43 N·m | 32 lb ft
Starter Solenoid Assembly Screws | 8 N·m | 71 lb in
Starter Solenoid Nuts | 15 N·m | 11 lb ft
Starter Through-Bolts | 6 N·m | 53 lb in