For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel center panel. Refer to Instrument Panel Center Trim Panel Replacement .
2. Disconnect the electrical connector.
3. Depress the retaining tabs.
4. Remove the hazard warning switch (1) from the instrument panel center panel.

### Installation Procedure

1. Install the hazard warning switch (1) to the instrument panel center panel.
2. Connect the electrical connector.
3. Install the instrument panel center panel. Refer to Instrument Panel Center Trim Panel Replacement.