For 1990-2009 cars

## Electrical Center Identification Views Notchback

Table 1: | Fuse Block - Underhood Label Usage
Table 2: | Fuse Block - Underhood C1
Table 3: | Fuse Block - Underhood C2
Table 4: | Fuse Block - Underhood C3
Table 5: | Fuse Block - Underhood C4
Table 6: | Fuse Block - I/P Label Usage
Table 7: | Fuse Block - I/P C1
Table 8: | Fuse Block - I/P C2
Table 9: | Fuse Block - I/P C3

### Fuse Block - Underhood

#### Fuse Block - Underhood Label Usage

Device | Rating | Description
--- | --- | ---
Ef1 | 50A | BATT
Ef2 | 20A/30A | P/Window 1
Ef3 | 30A | IGN2/ST
Ef4 | 30A | ACC/IGN1
Ef5 | -- | Not Used
Ef6 | -- | Not Used
Ef7 | 10A | P/Window 2
Ef8 | 10A | PK/LP LH
Ef9 | 10A | PK/LP RH
Ef10 | -- | Not Used
Ef11 | 15A | Fuel Pump
Ef12 | 10A | ECU
Ef13 | 15A | Engine Management System 1
Ef14 | 15A | Engine Management System 2
Ef15 | 15A | Hazard
Ef16 | -- | Not Used
Ef17 | 20A | Spare
Ef18 | 15A | Spare
Ef19 | 10A | Spare
Ef20 | 10A | H/L Low RH
Ef21 | 10A | H/L Low LH
Ef22 | 15A | FRT Fog
Ef23 | 15A | H/L High
Ef24 | 20A | Fan Low
Ef25 | 10A | A/C Compressor
Ef26 | 20A | Fuel Pump Relay
Ef27 | 35A | P/Window Relay
Ef28 | 20A | Park Lamp Relay
Ef29 | 20A | FRT Fog Relay
Ef30 | 20A | H/L High Relay
Ef31 | 20A | H/L Low Relay
Ef32 | 35A | Fan Hi Relay
Ef33 | 20A | Fan Low Relay
Ef34 | 20A | A/C Relay
Ef35 | 35A | Main Relay

### Fuse Block - Underhood (Bottom View)

#### Fuse Block - Underhood C1

Connector Part Information |

• | 1-936321-2

• | 32-Way F 090 SPT Hybrid Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | -- | Fuel Gage Sensor Signal - Right
2 | L-BU | -- | Low Reference
3 | OG/BK | -- | 5-Volt Reference
BN/BK
4 | OG/BK | -- | 5-Volt Reference
5 | PU | -- | Ignition 1 Voltage
6 | -- | -- | Not Used
7 | OG | -- | Ignition 1 Voltage
8 | BN | -- | HO2S2 Signal
9 | L-BU | -- | HO2S2 Low Reference
10 | BN | -- | HO2S2 Control
11 | BN/WH | -- | Fuel Gage Sensor Signal
12 | L-BU | -- | Low Reference
13 | OG/BK | -- | 5-Volt Reference
14 | YE | -- | Low Beam Headlamp Feed - Left
15 | PU/WH | -- | Air Conditioning Compressor Clutch Coil Enable Signal
16 | BN | -- | Vehicle Speed Signal
17 | RD/WH | -- | Battery Voltage
18 | OG/BK | -- | Ignition 1 Voltage
19 | OG/BK | -- | Ignition 1 Voltage
20 | OG | -- | Ignition 1 Voltage
21 | OG | -- | Ignition 1 Voltage
22 | -- | -- | Not Used
23 | L-GN | -- | Fuel Pump Relay Control
24 | OG/BK | -- | Ignition 1 Voltage
25 | BK/WH | -- | Ground
26 | OG/BK | -- | Ignition 1 Voltage
27 | PU | -- | Ignition 1 Voltage
28 | BN | -- | Main Relay Control
29 | PK | -- | Ignition 1 Voltage (Sirius D4)
30 | PK | -- | Ignition 1 Voltage
31 | BU | -- | Vehicle Speed Signal
32 | GY/GN | -- | Power Door Lock Anti-Lockout Relay Feed-Coil

#### Fuse Block - Underhood C2

Connector Part Information |

• | 2-936331-3

• | 32-Way F 090 SPT Hybrid Series (GY)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | PK | -- | Ignition 1 Voltage
4 | RD/BK | -- | Battery Voltage
5-6 | -- | -- | Not Used
7 | RD/BK | -- | Battery Voltage
RD/BK
8 | -- | -- | Not Used
9 | WH | -- | Headlamp Relay Coil Supply Voltage
10 | RD/BK | -- | TCM Signal Voltage
11 | D-BU | -- | Turn Signal Supply Voltage
12 | L-BU | -- | Turn Signal Supply Voltage
13 | L-BU | -- | Turn Signal Supply Voltage
14 | PU | -- | Power Window Relay Coil
15 | BN/WH | -- | Position Illumination Voltage
16 | BN/WH | -- | Position Illumination Voltage
17 | L-BU | -- | Headlamp High Relay Coil
18 | RD/WH | -- | Battery Voltage
19 | -- | -- | Not Used
20 | D-GN/WH | -- | Front Fog Lamp Signal
21 | PK | -- | Ignition 1 Voltage
22 | PK | -- | Ignition 1 Voltage
23-24 | -- | -- | Not Used
25 | YE | -- | Fog Lamp Relay Output - Common Contact
26 | RD/BK | -- | Battery Voltage
27 | WH | -- | Park Lamp Relay Output-Coil
28 | L-GN/BK | -- | Battery Voltage
29 | BN | -- | ABS Pulse Width Modulated Solenoid Feed - Rear
30 | L-GN/BK | -- | Battery Voltage
31-32 | -- | -- | Not Used

#### Fuse Block - Underhood C3

Connector Part Information |

• | 3-936321-4

• | 32-Way F 090 SPT Hybrid Series (BN)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BU | -- | Turn Signal Lamp Feed - Right Front
2 | BU | -- | Turn Signal Lamp Feed - Right Front
3 | RD/WH | -- | Battery Voltage
4 | YE | -- | Fog Lamp Relay Output - Common Contact
5 | L-GN/BK | -- | High Beam Headlamp Feed - Right
6 | BN/WH | -- | Low Beam Headlamp Feed - Right
7 | YE | -- | Low Beam Headlamp Feed - Left
8 | PU | -- | Park Lamp Feed - Left
9 | BN | -- | Wheel Speed Sensor Signal - Left Front
10 | -- | -- | Not Used
11 | BU | -- | Turn Signal Lamp Feed - Right Front
12-13 | -- | -- | Not Used
14 | PU | -- | Park Lamp Feed - Left
15 | -- | -- | Not Used
16 | BN | -- | Oxygen Sensor Return - Right - Rear of Catalytic Converter
17 | -- | -- | Not Used
18 | BK | -- | Ground
19 | BK | -- | Ground
20 | OG | -- | Electronic Control Unit Output - 12-Volt Inadvertent Load Control
21 | YE | -- | Low Beam Headlamp Feed - Left
22 | PU | -- | Oxygen Sensor Signal - Right - Rear of Catalytic Converter
23 | BK | -- | Ground
24 | BK | -- | Ground
25 | BN/WH | -- | Park Lamp Feed - Right
26 | GN/WH | -- | High Beam Headlamp Feed - Left
27 | GY | -- | Coolant Fan Motor Feed - Secondary
28 | L-BU | -- | Coolant Fan Motor Feed
29 | OG/BK | -- | Reference Voltage Feed - 12-Volt Reference
30 | PK | -- | Ignition 1
31 | PK | -- | Ignition 1
32 | BN | -- | Oxygen Sensor Return

#### Fuse Block - Underhood C4

Connector Part Information |

• | MG651068

• | 2-Way F 375 Series (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | -- | ABS Module Supply Voltage
2 | RD | -- | ABS Module Supply Voltage

### Fuse Block - I/P Label

#### Fuse Block - I/P Label Usage

Device | Rating | Description
--- | --- | ---
F1 | 10A | SDM
F2 | 25A | Wiper
F3 | 10A | Cluster
F4 | 10A | T/SIG
F5 | 10A | EMS2
F6 | 15A | EMS1
F7 | 15A | Stop Lamp
F8 | 15A | Cigar
F9 | 10A | Audio/Clock
F10 | 10A | OBD
F11 | -- | Not Used
F12 | 10A | Room Lamp
F13 | 25A | Defogger
F14 | 20A | Sunroof
F15 | 10A | RR Fog
F16 | 15A | Door Lock
F17 | 10A | B/UP Lamp
F18 | 10A | Horn
F19 | 10A | Elec Mirror
F20 | 10A | Defog Mirror
F21 | 15A | Audio/RKE

### Fuse Block - I/P (Bottom View)

#### Fuse Block - I/P C1

Connector Part Information |

• | 936195-1

• | 76-Way F 090/250 Hybrid Series (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 641 | Ignition 2 Voltage
2 | BN | 641 | Ignition 2 Voltage
BN | 641 | Ignition 2 Voltage
3 | BN/WH | 309 | Illumination Feed
4-7 | -- | -- | Not Used
8 | L-BU | 74 | Park Lamp Switch Output
9 | -- | -- | Not Used
10 | RD/WH | 540 | Battery Positive Voltage
11 | -- | -- | Not Used
12 | BK | 450 | Ground
13 | -- | -- | Not Used
14 | L-GN | 1076 | Key Interlock Solenoid
15 | OG | 122 | Fog Lamp Indicator Feed - Rear
16-17 | -- | -- | Not Used
18 | BN | 33 | Brake Warning Indicator Lamp Output
19 | -- | -- | Not Used
20 | WH | 629 | Cluster C2
21 | D-GN/WH | 900 | Key Illumination Low Reference
22 | RD/WH | 540 | Battery Positive Voltage
23 | RD/WH | 540 | Battery Positive Voltage
RD/WH | 540 | Battery Positive Voltage
24 | BN | 31 | Oil Pressure Indicator Lamp Output
25 | L-GN | 80 | Key Reminder Switch Signal
26 | WH | 193 | Rear Defogger Relay Control
27 | RD/WH | 640 | Battery Voltage
28-29 | -- | -- | Not Used
30 | L-BU | 97 | Windshield Wiper Switch Signal - Mist/Off/Low
31 | GY | 91 | Windshield Wiper Relay Feed-Coil
32 | -- | -- | Not Used
33 | RD/WH | 540 | Battery Positive Voltage
RD/WH | 540 | Battery Positive Voltage
34 | BN/WH | 238 | Seat Belt Switch Signal
BN/WH | 238 | Seat Belt Switch Signal (-AJ3)
35 | -- | -- | Not Used
36 | OG | 300 | Ignition Switch Output - Ignition 2 Voltage
37 | L-GN | 1845 | Multifunction Chime Control Signal
38 | BN | 841 | Ignition 2 Voltage
BN | 841 | Ignition 2 Voltage
39 | D-GN | 29 | Horn Relay Control
D-GN | 29 | Horn Relay control
40 | -- | -- | Not Used
41 | RD/WH | 240 | Battery Positive Voltage
RD/WH | 240 | Battery Positive Voltage
42 | -- | -- | Not Used
43 | YE | 356 | Power Door Lock Relay Feed-Coil Driver Door Unlock
44 | GY/D-GN | 355 | Power Door Lock Anti-Lockout Relay Feed-Coil
45 | RD/WH | 1340 | Battery Positive Voltage
46 | RD/WH | 1340 | Battery Voltage - Folding Mirror
47 | YE | 143 | Accessory Voltage
48-49 | -- | -- | Not Used
50 | WH | 156 | Courtesy Lamp Output
WH | 156 | Courtesy Lamp Output
51-52 | -- | -- | Not Used
53 | BN | 1075 | Ignition Key Cylinder Solenoid Lock Enable
54 | L-BU | 292 | Rear Defogger Switch Signal - Primary
55 | YE | 1977 | Fog Lamp Relay Output-Coil - Rear
56 | PK | 239 | Ignition 1 Voltage
PK | 239 | Ignition 1 Voltage
57 | OG/BK | 434 | Neutral Safety Switch
58 | RD/WH | 1340 | Battery Positive Voltage
59 | -- | -- | Not Used
60 | YE | 43 | Accessory Voltage
YE | 43 | Accessory Voltage
61 | YE | 43 | Accessory Voltage
62 | PK | 139 | Ignition 1 Voltage
63-64 | -- | -- | Not Used
65 | PK | 639 | Ignition 1 Voltage
66 | RD/WH | 340 | Battery Positive Voltage
67 | PK | 822 | Vehicle Speed Sensor Signal
68 | PK | 239 | Ignition 1 Voltage
PK | 239 | Ignition 1 Voltage
PK | 239 | Ignition 1 Voltage
69 | PK | 239 | Ignition 1 Voltage
PK | 1739 | Ignition 1 Voltage (PPS)
70 | PK | 239 | Ignition 1 Voltage
71 | BK/WH | 1352 | Dual Zone Switch Signal-Offset
72 | PK | 339 | Ignition 1 Voltage
73 | PK | 3 | Ignition Switch Output - Ignition 1
74 | BN | 4 | Ignition Switch Output - Accessory
75 | -- | -- | Not Used
76 | L-BU | 195 | Power Door Lock Relay Feed - Lock Coil

#### Fuse Block - I/P C2

Connector Part Information |

• | 368457-1

• | 20-Way F (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | -- | Battery Positive Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | WH | -- | Courtesy Lamp Output
4 | BN/WH | -- | Brake Warning Indicator Lamp Output
5 | -- | -- | Not Used
6 | WH | -- | Power Door Lock Relay Feed - Unlock Coil
7 | -- | -- | Not Used
8 | GY | -- | Power Door Lock Motor Feed - Lock
9 | OG | -- | Heated Mirror Element Feed
10 | PK | -- | Ignition 1 Voltage
11 | GY | -- | Interior Lamp Output
12 | -- | -- | Not Used
13 | YE | -- | Accessory Voltage
14 | -- | -- | Not Used
15 | OG | -- | Rear Defog Relay Output
16 | OG | -- | Fog Lamp Feed - Rear
17 | WH | -- | Courtesy Lamp Output
18 | L-BU | -- | Power Door Lock Relay Feed - Lock Coil
19 | -- | -- | Not Used
20 | BN | -- | Power Door Lock Motor Feed - Unlock

#### Fuse Block - I/P C3

Connector Part Information |

• | 368497-1

• | 18-Way M (WH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | -- | Power Window Enable Relay Output - N.O. Contact
2 | WH | -- | Park Lamp Relay Output-Coil
3 | PK | -- | Windshield Washer Switch Signal
4 | L-BU | -- | Stop Lamp Signal (LHD)
5 | PK | -- | Ignition 1 Voltage
6 | BN/WH | -- | Brake Warning Indicator Lamp Output
7 | -- | -- | Not Used
8 | BN | -- | Horn Relay Output-Coil
9 | BN/WH | -- | Park Lamp Feed-Right
10 | D-GN/WH | -- | Fog Lamp Relay Output-Coil
D-GN/WH
11 | WH | -- | Headlamp Relay Feed - Coil
12 | PK | -- | Ignition 1 Voltage
13 | RD/BK | -- | Battery Voltage
14 | BN | -- | Windshield Wiper Motor Feed - Low Speed
15 | GN/BK | -- | Ignition 1 Voltage
16 | PK | -- | Ignition 1 Voltage
17 | PK | -- | Ignition 1 Voltage
18 | -- | -- | Not Used

## Electrical Center Identification Views Hatchback

Table 1: | Fuse Block - Underhood Label Usage
Table 2: | Fuse Block - Underhood Wire Entry
Table 3: | Fuse Block - I/P Label Usage
Table 4: | Fuse Block I/P Wire Entry

### Fuse Block - Underhood Label (1.4L/1.5L)

### Fuse Block - Underhood Label (1.2L/1.6L)

#### Fuse Block - Underhood Label Usage

Device | Rating | Description
--- | --- | ---
PWR WNDW Fuse (EF1) | 30A | PWR WNDW Relay
MAIN RELAY Fuse (EF2) | 20A | MAIN POWER Relay (1.2L)
COOL FAN Fuse (EF3) | 30A | COOL FAN HI Relay and COOL FAN LOW Relay
ABS Fuse (EF4) | 60A | Electronic Brake Control Module (EBCM)
IGN 1 Fuse (EF5) | 30A | Ignition Switch
IGN 2 Fuse (EF6) | 30A | Ignition Switch
I/P FUSE BATT. Fuse (EF7) | 30A | CLK RADIO Fuse, CLSTR HAZRD Fuse, ECM TCM Fuse, DR/LCK Fuse, HORN REAR/FOG Fuse and STOP Fuse
HVAC BLOWER Fuse (EF8) | 20A | Blower Relay
FOG LAMPS Fuse (EF9) | 15A | FRT FOG Relay
FUEL Fuse (EF10) | 15A | FUEL PUMP Relay
HORN Fuse (EF11) | 10A | Horn, Hood Ajar Switch, and Theft Deterrent Alarm
S/ROOF Fuse (EF12) | 20A | Sunroof Module
INJECTOR Fuse (EF13) (1.6L) | 10A | Camshaft Position (CMP) Sensor, COOL FAN HI Relay, COOL FAN LOW Relay, Engine Control Module (ECM), Exhaust Gas Recirculation (EGR) Valve, Fuel Injector 1-4, and Intake Manifold Tuning Valve
ILLUM LT Fuse (EF14) | 10A | License Lamp, Park Position Lamp - Left (Except North America), Park/Turn Signal Lamp - LF, Side Marker Lamp - LF, Side Marker Lamp - LR, Side Marker Lamp - RR, and Tail/Stop Lamp - Left
ILLUM RT Fuse (EF15) | 10A | Ashtray Lamp, Clock, Defogger Switch, DRL Control Module, DRL Relay, Fog Lamp Switch - Front, Fog Lamp Switch - Rear, Hazard Switch, HVAC Control, Instrument Cluster, Multifunction Alarm Module, Park Position Lamp - Right (Except North America), Park/Turn Signal Lamp - RF, Radio, Shift Indicator Lamp, Side Marker Lamp - RF, and Tail/Stop Lamp - Right
DIODE (FOG) (EF16) | -- | HI BEAM RT Fuse
DIS Fuse (EF17) (1.6L) | 10A | A/C CMPRSR Relay, Engine Control Module (ECM), EVAP Canister Purge Solenoid Valve, Heated Oxygen Sensor 1 (HO2S1), Heated Oxygen Sensor 2 (HO2S2), and Ignition Coil Module
A/C Fuse (EF18) | 20A | A/C CMPRSR Relay
HEAD LAMPS Fuse (EF19) | 25A | DRL Module, HEAD LAMPS LOW Relay, and HEAD LAMPS HI Relay
ILLUM LAMPS Fuse (EF20) | 20A | ILLUM LAMPS Relay
DEFOG Fuse (EF21) | 30A | Defog Relay
INT LTS Fuse (EF22) | 10A | Courtesy/Reading Lamp (w/o Sunroof), Rear Compartment Lamp, and Sunroof Switch (w/Sunroof)
LOW BEAM LT Fuse (EF23) | 10A | Headlamp Leveling Motor - LH and Headlamp Low Beam - Left
LOW BEAM RT Fuse (EF24) | 10A | Headlamp Leveling Motor - RH and Headlamp Low Beam - Right
HI BEAM LT Fuse (EF25) | 10A | Headlamp High Beam - Left
HI BEAM RT Fuse (EF26) | 10A | Headlamp High Beam - Right
A/C CMPRSR Relay | -- | A/C Compressor Clutch and Engine Control Module (ECM)
COOL FAN CNTROL Relay (1.4L, 1.5L)) | -- | Cooling Fan - Auxiliary
COOL FAN HI Relay | -- | Cooling Fan Resistor (1.2L, 1.6L), Cooling Fan (1.2L, 1.6L), Cooling Fan - Main (1.4L, 1.5L) and Engine Control Module (ECM)
COOL FAN LOW Relay | -- | Cooling Fan Resistor (1.2L, 1.6L), Cool Fan - Auxiliary (1.4L, 1.5L) and Engine Control Module (ECM)
FRT FOG Relay | -- | Fog Lamp - LF, Fog Lamp - RF, and Headlamp
FUEL PUMP Relay | -- | Engine Control Module (ECM), Fuel Pump
HEAD LAMPS HI Relay | -- | HIGH BEAM LT Fuse, HIGH BEAM RT Fuse, Turn Signal Swtich
HEAD LAMPS LOW Relay | -- | Daytime Running Lamp (DRL) Module, Engine Control Module (ECM), Headlamp Leveling Switch, LOW BEAM LT Fuse, LOW BEAM RT Fuse, Rear Fog Diode
ILLUM LAMPS Relay | -- | ILLUM LT Fuse, ILLUM RT Fuse, Lamp Control Module
MAIN POWER Relay (1.2L/1.6L) | -- | Engine Control Module (ECM), Camshaft Position Sensor (CMP) (1.2L), Heated Oxygen Sensor 1 (HO2S1) (1.2L), Heated Oxygen Sensor 2 (HO2S2) (1.2L), Fuel Injector 1-4 (1.2L), DIS Fuse (1.6L), INJECTOR Fuse (1.6L)
PWR WNDW Relay | -- | Power Window Switch - Driver, Power Window Switch - Passenger (A32)

### Fuse Block - Underhood Top View

### Fuse Block - Underhood Bottom View

#### Fuse Block - Underhood Wire Entry

Connector Part Information |

• | 96539834

• | 97-Way F Fuse Block (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/YE | 2100 | Ignition 2 Voltage (1.4L, 1.5L, 1.6L)
BN | 1541 | Ignition 1 Voltage (1.2L)
2 | BN | 409 | Cooling Fan Motor Supply Voltage
3 | RD | 532 | Cooling Fan Motor Supply Voltage
4 | D-GN | 335 | Low Speed Cooling Fan Relay Control
5 | BN | 1541 | Ignition 1 Voltage
6 | YE/D-GN | 712 | Left Headlamp Low Beam Supply Voltage
7 | PK | 39 | Battery Positive Voltage
PK | 39 | Battery Positive Voltage
8 | WH | 352 | Headlamp Relay Coil Supply Voltage
9 | WH/YE | 318 | Front Fog Lamp Supply Voltage (T96)
10 | L-BU | 1769 | Fog Lamp Switch Supply Voltage (T96)
11 | OG | 1740 | Battery Positive Voltage (T96)
12 | BK | 50 | Ground (T96)
L-GN | 319 | Left Hand High Beam Supply Voltage (North America w/T96)
13 | YE/BK | 497 | Fuel Pump Relay Control
14 | OG | 1940 | Battery Positive Voltage
15 | L-BU | 1723 | Fuel Pump Supply Voltage
16 | BK | 50 | Ground (1.4L, 1.6L)
17 | D-GN | 67 | A/C Compressor Clutch Coil Supply Voltage (C60)
18 | L-BU/BK | 812 | A/C Compressor Clutch Supply Voltage (C60)
19 | D-GN | 59 | Battery Positive Voltage (C60)
20 | L-GN | 459 | Ignition 3 Voltage (C60)
21 | BN | 9 | Battery Positive Voltage
22 | L-BN | 74 | Park Lamp Switch Signal
L-BN | 74 | Park Lamp Switch Signal
23 | BN | 9 | Battery Positive Voltage
24 | BN | 1080 | Park Lamp Relay Control
25 | WH/BK | 1346 | Headlamp Relay Supply Voltage
26 | -- | -- | Not Used
27 | PK | 39 | Battery Positive Voltage
28 | GY/D-GN | 711 | Left Headlamp High Beam Supply Voltage
29 | -- | -- | Not Used
30 | BN | 1541 | Ignition 3 Voltage
31 | BK | 150 | Ground
32 | -- | -- | Not Used
33 | OG | 542 | Battery Positive Voltage
34 | BN | 41 | Battery Positive Voltage
35 | -- | -- | Not Used
36 | D-GN/YE | 2100 | Ignition 3 Voltage
37 | GY | 473 | High Speed Cooling Fan Relay Control (1.4L, 1.5L, 1.6L)
BN | 1741 | Main Relay Coil Supply Voltage
38 | PU | 532 | Cooling Fan Motor Supply Voltage (1.4L, 1.5L, 1.6L)
39 | BK | 150 | Ground (1.4L, 1.5L, 1.6L)
BN | 409 | Battery Positive Voltage (1.2L)
BN | 409 | Battery Positive Voltage (1.2L)
40 | L-BU | 504 | Accessory Voltage (w/Dual Fans) (1.4L, 1.5L, 1.6L)
D-GN/YE | 2100 | Ignition 3 Voltage (1.2L)
41 | -- | -- | Not Used
42 | D-GN/YE | 2100 | Ignition 3 Voltage (1.4L, 1.5L, 1.6L)
BN | 409 | Battery Positive Voltage
43 | GY | 473 | High Speed Cooling Fan Relay Control (w/Dual Fans) (1.4L, 1.5L, 1.6L)
44 | -- | -- | Not Used
45 | RD | 532 | Battery Positive Voltage
46 | PU | 532 | Battery Positive Voltage
PU | 532 | Battery Positive Voltage (w/Dual Fans)
47 | -- | -- | Not Used
48 | D-GN/YE | 2100 | Ignition 3 Voltage
49 | OG | 542 | Battery Positive Voltage
50 | BN | 409 | Battery Positive Voltage (1.2L)
51 | RD | 532 | Battery Positive Voltage
52 | RD | 42 | Battery Positive Voltage
53 | OG | 1740 | Battery Positive Voltage
54 | OG | 1940 | Battery Positive Voltage
55 | OG | 1440 | Battery Positive Voltage
OG | 1440 | Battery Positive Voltage (w/RKE)
BN | 641 | Battery Positive Voltage (w/RKE and Siren)
56 | BN | 741 | Battery Positive Voltage
57 | -- | -- | Not Used
58 | PU/WH | 709 | Left Park Lamp Supply Voltage
59 | PU/WH | 309 | Right Park Lamp Supply Voltage
60-61 | -- | -- | Not Used
62 | -- | -- | Battery Positive Voltage - BUS
63 | -- | -- | Battery Positive Voltage - BUS
64 | -- | -- | Battery Positive Voltage - BUS
65 | -- | -- | Battery Positive Voltage - BUS
66 | -- | -- | Battery Positive Voltage - BUS
67 | -- | -- | Battery Positive Voltage - BUS
68 | -- | -- | Battery Positive Voltage - BUS
69 | -- | -- | Battery Positive Voltage - BUS
70 | -- | -- | Not Used
71 | L-BU | -- | Left Park Lamp Supply Voltage - BUS
72 | L-BU | 74 | Park Lamp Switch Signal
73-74 | -- | -- | Not Used
75 | -- | -- | Battery Positive Voltage
76 | RD/BK | 141 | Battery Positive Voltage
77 | OG/BK | 142 | Battery Positive Voltage
78 | YE | 143 | Battery Positive Voltage
79 | RD/BK | 141 | Battery Positive Voltage
80 | D-GN | 59 | Battery Positive Voltage
81 | OG | 140 | Battery Positive Voltage (1.4L, 1.5L, 1.6L)
PK | 39 | Battery Positive Voltage
BN | 140 | Battery Positive Voltage (1.2L - LHD)
82 | BN | 9 | Battery Positive Voltage
83 | OG/D-GN | 1142 | Battery Positive Voltage
84 | OG/BK | 540 | Battery Positive Voltage
85 | PU/WH | 312 | Left Headlamp Low Beam Supply Voltage
PU/WH | 312 | Left Headlamp Low Beam Supply Voltage (w/Headlamp Leveling)
86 | YE | 712 | Right Headlamp Low Beam Supply Voltage
YE | 712 | Right Headlamp Low Beam Supply Voltage (w/Headlamp Leveling)
87 | PU | 311 | Left Headlamp High Beam Supply Voltage
88 | GY | 711 | Right Headlamp High Beam Supply Voltage
89 | -- | -- | Battery Positive Voltage - BUS
90 | -- | -- | Battery Positive Voltage - BUS
91 | -- | -- | Battery Positive Voltage - BUS
92 | -- | -- | Battery Positive Voltage - BUS
93 | -- | -- | Battery Positive Voltage - BUS
94 | -- | -- | Battery Positive Voltage - BUS
95 | -- | -- | Battery Positive Voltage - BUS
96 | OG | 40 | Battery Positive Voltage
97 | OG | 40 | Battery Positive Voltage
98 | -- | -- | Right Headlamp High Beam Supply Voltage BUS
99 | YE/D-GN | 712 | Right Headlamp Low Beam Supply Voltage
100 | -- | -- | Right Headlamp High Beam Supply Voltage BUS
101 | GY/D-GN | 711 | Right Headlamp High Beam Supply Voltage

### Fuse Block - I/P Label

#### Fuse Block - I/P Label Usage

Device | Rating | Description
--- | --- | ---
F1 - LTR | 15A | Cigar Lighter, Extra Power Jack
F2 - RADIO CLK | 10A | Radio, Clock
F3 - TRN/51G | 15A | Hazard Switch
F4 - CLSTR CLK | 10A | DRL, Clock, Cluster, Chime Bell, Immobilizer
F5 - BCK/UP | 10A | Backup Switch
F6 - ECM/TCM | 10A | VSS, ECM, TCM, PNP Switch
F7 - DIS INJECTOR | 15A | ABS Warning Lamp Module
F8 - AIR BAG | 10A | SDM
F9 | 10A | ABS
F10-F11 | -- | Not Used
F12 - HORN REAR/FOG | 10A | Horn Relay, Key Remind Switch, DRL Relay
F13 - STOP | 15A | Brake Switch
F14 - CLSTR HAZARD | 15A | Cluster, Blink Relay, Hazard Switch
F15 - DRL/LCK | 15A | Central Door Lock Unit, Anti-Theft Module
F16 - ECM/TCM | 10A | Immobilizer, DLC, TCM, ECM
F17 - WPR WSW | 20A | Windshield Wiper, Wiper Relay, Wiper Switch, Room Lamp
F18 - ABS ENG FUSE | 10A | EBCM, Power Window Relay, A/C Switch, Cooling Fan
F19 - HVAC | 20A | Blower Switch, A/C Switch, Defog Switch
F20 | -- | Not Used
F21 | -- | ABS Diode
F22 | -- | Not Used
F23 - CLK RADIO | 10A | Radio, Clock

### Fuse Block - I/P Top View

### Fuse Block - I/P Bottom View

#### Fuse Block I/P Wire Entry

Connector Part Information |

• | 96539835

• | 46-Way F Fuse Block (BK)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 340 | Battery Positive Voltage (w/Air Bag)
RD | 122 | Rear Fog Lamp Supply Voltage (w/Rear Fog Lamps)
OG | 340 | Battery Positive Voltage (w/RKE)
OG | 340 | Battery Positive Voltage (w/DRL - Scandinavia)
2 | OG | 540 | Battery Positive Voltage
3 | OG | 640 | Battery Positive Voltage
YE | 1040 | Battery Positive Voltage
OG | 640 | Battery Positive Voltage (w/Lamp Driver Module)
4 | OG | 1340 | Battery Positive Voltage (w/Power Door Locks)
5 | OG | 240 | Battery Positive Voltage (w/Immobilizer)
OG | 440 | Battery Positive Voltage
OG | 440 | Battery Positive Voltage (w/OBD)
6 | RD | 441 | Ignition 3 Voltage
7 | RD/BK | 1541 | Ignition 1 Voltage
8 | YE | 343 | Accessory Voltage
9 | BN | -- | Not Used
10 | BN | 233 | Brake Warning Indicator Control (LHD)
11 | -- | -- | Not Used
12 | OG | 143 | Battery Positive Voltage
OG | 143 | Battery Positive Voltage
13 | OG | 143 | Battery Positive Voltage - BUS
14 | OG | 143 | Battery Positive Voltage - BUS
15 | OG | 143 | Battery Positive Voltage - BUS
16 | OG | 143 | Battery Positive Voltage - BUS
OG | 143 | Battery Positive Voltage - BUS
OG | 143 | Battery Positive Voltage - BUS
17 | RD | 341 | Ignition 3 Voltage
18 | BN | 341 | Ignition 3 Voltage - BUS
19 | YE | 341 | Ignition 3 Voltage - BUS
20 | -- | -- | Not Used
21 | BN/WH | 133 | Brake Warning Indicator Control (LHD)
22 | -- | -- | Not Used
23 | OG | 40 | Accessory Voltage
24 | YE | 43 | Accessory Voltage
YE | 43 | Accessory Voltage
YE | 43 | Accessory Voltage (North American w/Automatic Transmission)
YE | 43 | Accessory Voltage (North American w/Automatic Transmission)
25 | PK | 339 | Ignition 1 Voltage
26 | PK | 239 | Ignition 1 Voltage
27 | PK | 439 | Ignition 1 Voltage
PK | 439 | Ignition 1 Voltage (North American w/Automatic Transmission)
28 | PK | 1739 | Ignition 1 Voltage
29 | PK | 539 | Ignition 1 Voltage
PK | 241 | Ignition 1 Voltage (w/ABS)
30 | PK | 139 | Ignition 1 Voltage (w/Airbag) (LHD)
OG | 139 | Ignition 1 Voltage (w/Airbag) (RHD)
31-33 | -- | -- | Not Used
34 | YE | 4 | Accessory Voltage
35 | -- | 4 | Accessory Voltage - BUS
36 | PK | 3 | Ignition 1 Voltage
37 | PK | 3 | Ignition 1 Voltage - BUS
38 | -- | 3 | Ignition 1 Voltage - BUS
39 | -- | 3 | Ignition 1 Voltage - BUS
40 | -- | 3 | Ignition 1 Voltage - BUS
41 | -- | 3 | Ignition 1 Voltage - BUS
42 | -- | 3 | Ignition 1 Voltage - BUS
43-44 | -- | -- | Not Used
45 | YE/BK | 143 | Battery Positive Voltage
46 | OG | 540 | Battery Positive Voltage