For 1990-2009 cars

## High Mount Stop Lamp Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the rear deck lid.
3. Remove the screws and the center high-mounted stop lamp (CHMSL).
4. Remove the CHMSL bulb.

### Installation Procedure

1. Install the CHMSL bulb.
2. Install the CHMSL with the screws.
3. Connect the negative battery cable.

## High Mount Stop Lamp Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open the hatchback door.
3. Pry open the center high-mounted stop lamp (CHMSL) access cover with a screwdriver.
4. Disconnect the electrical connector.
5. Remove the screws and the CHMSL.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CHMSL with the screws.

Tighten
Tighten the CHMSL mounting screws to 3 N·m (27 lb in).

2. Connect the electrical connector.
3. Close the CHMSL access cover.
4. Connect the negative battery cable.