For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the front wheel speed sensor electrical connector.

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

3. Raise and suitably support the vehicle.
4. Remove the bolt and the front wheel speed sensor from the steering knuckle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the bolt and front wheel speed sensor to the steering knuckle.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

2. Lower the vehicle.
3. Connect the front wheel speed sensor electrical connector.
4. Connect the negative battery cable.