For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Gently pry the luggage compartment lamp off by inserting a flathead screwdriver into the recess on the edge of the lamp.
3. Disconnect the electrical connector.
4. Remove the bulb.

### Installation Procedure

1. Install a new bulb.
2. Connect the electrical connector.
3. Insert the luggage compartment lamp into the recess and press the lens into place.
4. Connect the negative battery cable.