For 1990-2009 cars

### Removal Procedure

1. Open the hatchback door.
2. Remove the hatchback door lower garnish molding.
3. Remove the screws and the hatchback lock.
4. Disconnect the lock rods and the electrical connector.

### Installation Procedure

1. Connect the lock rods and the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hatchback lock with the screws.

Tighten
Tighten the hatchback door lock screws to 6 N·m (53 lb in).

3. Install the hatchback door lower garnish molding.
4. Close the hatchback door.