For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the lower steering column cover panel screws.
3. Turn the steering wheel to expose the upper steering column cover panel connecting screws. Remove the upper steering column cover panel screws and remove the upper steering column cover panel.
4. Remove the wiper switch by pushing in on the tabs on either side of the switch housing.
5. Disconnect the electrical connections from the wiper switch.

### Installation Procedure

1. Connect the electrical connections to the wiper switch.
2. Install the wiper switch by snapping it into the switch housing.
3. Install the upper and lower steering column panels.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the lower steering column panel screws.

Tighten
Tighten the lower steering column cover panel screws to 3 N·m (27 lb in).

5. Turn the steering wheel in order to access the upper steering column panel screws holes. Install the upper steering column cover panel screws.

Tighten
Tighten the upper steering column cover panel screws to 3 N·m (27 lb in).

6. Connect the negative battery cable.