For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the headlamps. Refer to Headlamp Replacement .
3. Disconnect the electrical connector.
4. Remove the side marker bulb from the headlamp assembly.
5. Remove the side marker bulb from the socket.

### Installation Procedure

1. Install the side marker bulb to the socket.
2. Install the side marker bulb into the headlamp assembly.
3. Connect the electrical connector.
4. Install the headlamp. Refer to Headlamp Replacement .
5. Connect the negative battery cable.