For 1990-2009 cars

## Rear License Plate Lamp Replacement Typical

### Removal Procedure

1. Remove the screws.
2. Disconnect the electrical connector.
3. Remove the lamp assembly.
4. Remove the bulb.

### Installation Procedure

1. Install a new bulb.
2. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lamp assembly with the screws.

Tighten
Tighten the license plate lamp screws to 1.5 N·m (13 lb in).