For 1990-2009 cars

#### Special Tools

KM-210-A Steering Wheel Puller

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the SIR module. Refer to Inflatable Restraint Steering Wheel Module Replacement.
3. Place match marks on the steering wheel and on the steering column shaft.
4. Disconnect the horn connector.
5. Remove the steering wheel nut (4) and the retaining clip.
6. Remove the steering wheel using the KM-210-A .
7. Unclip the contact ring from the steering wheel, if necessary.

### Installation Procedure

1. Clip the contact ring on the steering wheel, if necessary.
2. Align the match marks on the steering wheel and the steering column shaft. Turn the signal-canceling cam on the wheel to the left.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the retaining clip and the steering wheel nut (4).

Tighten
Tighten the steering wheel nut to 38 N·m (28 lb ft).

4. Bend the tabs to secure the retaining clip.
5. Install the SIR module. Refer to Inflatable Restraint Steering Wheel Module Replacement.
6. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.