For 1990-2009 cars

## Seat Cushion Outer Trim Panel Replacement Dial Type

### Removal Procedure

1. Remove the front bucket seat from the vehicle. Refer to Front Seat Replacement - Bucket.
2. Remove the height adjustment knob. Refer to Front Seat Adjuster Replacement.
3. Remove the recliner adjustment knob.
4. Remove the screws and the front seat inner and outer cover from the seat.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front seat inner and outer cover with the screws and tighten to 12 N·m (106 lb in).
2. Install the recliner adjustment knob.
3. Install the height adjustment knob. Refer to Front Seat Adjuster Replacement.
4. Install the front bucket seat in the vehicle. Refer to Front Seat Replacement - Bucket.

## Seat Cushion Outer Trim Panel Replacement Lever Type

### Removal Procedure

1. Remove the front bucket seat from the vehicle. Refer to Front Seat Replacement - Bucket.
2. Remove the height adjustment knob. Refer to Front Seat Adjuster Replacement.
3. Remove the screw and reclining knob.
4. Remove the screws and the front seat inner and outer cover from the seat.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front seat inner and outer cover with the screws and tighten to 12 N·m (106 lb in).
2. Install the reclining knob.
3. Install the height adjustment knob. Refer to Front Seat Adjuster Replacement.
4. Install the front bucket seat in the vehicle. Refer to Front Seat Replacement - Bucket.