For 1990-2009 cars

## Compressor Relay Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. The relay is located in the fuse junction box in the engine compartment on the right-hand side.
3. Pull the relay straight up and out.

### Installation Procedure

1. Align the relay terminal contacts with the base receptacle.
2. Push the relay into the base until it is seated.
3. Connect the negative battery cable.

## Compressor Relay Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. The relay is located in the fuse junction box in the engine compartment on the right-hand side.
3. Pull the relay (1) straight up and out.

### Installation Procedure

1. Align the relay terminal contacts with the base receptacle.
2. Push the relay (1) into the base until it is seated.
3. Connect the negative battery cable.