For 1990-2009 cars

## Fascia Grille Replacement Notchback

### Removal Procedure

1. Open the hood.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
3. Remove the screws and the radiator grille.

### Installation Procedure

1. Install the radiator grille with the screws.
2. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .
3. Close the hood.

## Fascia Grille Replacement Hatchback

### Removal Procedure

1. Open the hood.
2. Remove the upper clips on the radiator grille.
3. Remove the radiator grille upper cover (1).
4. Remove the grille to front fascia clips (1).
5. Remove the radiator grille (2).
6. Remove the front fascia air guard clips (1), if necessary.
7. Remove the front fascia air guard (2) from the vehicle, if necessary.

### Installation Procedure

1. Install the front fascia air guard (2) to the vehicle, if removed.
2. Install the front fascia air guard clips (1), if removed.
3. Install the radiator grille (2).
4. install the grille to front fascia clips (1).
5. Install the radiator grille upper cover (1).
6. Install the upper clips on the radiator grille.
7. Close the hood.