For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat backs.
2. Remove the bolts that secure the rear seat backs to the hinges.
3. Remove the rear seat backs by pulling the seat hinge posts out of the lower rear quarter upper trim panel.

### Installation Procedure

1. Install the rear seatback by inserting the seat hinge posts into the lower rear quarter upper trim panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the seat backs to the hinges with the bolts.

Tighten
Tighten the seatback bolts to 25 N·m (18 lb ft).

3. Raise the rear seat backs in the upright position.