For 1990-2009 cars

### Removal Procedure

Caution: Refer to Fuel Pressure Caution in the Preface section.

1. Relieve the fuel pressure. Refer to Fuel Pressure Relief.

Warning: Refer to Battery Disconnect Warning in the Preface section.

2. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Disconnect the inlet/outlet fuel lines by moving the line connector lock forward and pulling the hose off of the fuel filter tube.
4. Remove the fuel filter bracket bolts (1).
5. Remove the fuel filter (2).

### Installation Procedure

1. Install the fuel filter (2).
2. Install the fuel filter bracket bolts (1).
3. Connect the inlet/outlet quick connector lines.
4. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.