For 1990-2009 cars

## Remote Control Door Lock Receiver Replacement Hatchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

Note: Remote keyless transmitters must be programmed when remote control module/receiver is replaced.

1. Disconnect the negative battery cable.
2. Remove the instrument panel storage compartment. Refer to Instrument Panel Storage Compartment Replacement.
3. Disconnect the control module/receiver electrical connector.
4. Slide the control module/receiver (1) away from its mounting bracket.

### Installation Procedure

1. Install the control module/receiver (1) on its mounting bracket.
2. Connect the control module/receiver electrical connector.
3. Install the instrument panel storage compartment. Refer to Instrument Panel Storage Compartment Replacement.
4. Connect the negative battery cable.
5. Complete remote keyless transmitter programming. Refer to Transmitter Programming.

## Remote Control Door Lock Receiver Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

Note: Remote keyless transmitters must be programmed when remote control module/receiver is replaced.

1. Disconnect the negative battery cable.
2. Separate the hood release cable from the hood latch release handle.
3. Carefully pull the instrument panel under cover until the mounting clips are released and the instrument panel under the cover.
4. Remove the bolts from the driver side knee bolster.
5. Disconnect the control module/receiver electrical connector.
6. Slide the control module/receiver away from its mounting bracket.

### Installation Procedure

1. Install the control module/receiver on its mounting bracket.
2. Connect the control module/receiver electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the knee bolster with bolts and tighten to 10 N m (89 lb in).
4. Install the instrument panel under cover.
5. Connect the hood release cable to the hood latch release handle.
6. Install the screws.
7. Connect the negative battery cable.
8. Complete remote keyless transmitter programmming. Refer to Transmitter Programming