For 1990-2009 cars

### Removal Procedure

1. Remove the rotor. Refer to Brake Rotor Replacement .
2. Remove the screws for the splash shield from the steering knuckle.
3. Remove the splash shield.

### Installation Procedure

1. Install the splash shield.

Notice: Refer to Fastener Notice in the Preface section.

2. Secure the splash shield to the steering knuckle with the screws.

Tighten
Tighten the splash shield-to-steering knuckle screws to 4 N·m (35 lb in).

3. Install the rotor. Refer to Brake Rotor Replacement .