For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the clutch control cable adjusting nut (1).
3. Remove the clutch control cable from the mounting bracket (2).
4. Disconnect the clutch control cable from the clutch pedal.
5. Remove the battery.
6. Remove the clutch control cable to cowl mounting nuts.
7. Remove the clutch control cable.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the clutch control cable to cowl and install the clutch control cable mounting nuts.

Tighten
Tighten the nuts 13 N·m (115 lb in).

2. Install the battery.
3. Connect the clutch control cable to the clutch pedal.
4. Install the clutch control cable to the mounting bracket (2).
5. Install the clutch control cable-adjusting nut (1).
6. Adjust the clutch control cable.