For 1990-2009 cars

### Removal Procedure

1. Remove the seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seat back. Refer to Rear Split Folding Seat Back Replacement .
3. Remove the rear rocker panel cover.
4. Remove the front wheelhouse trim.
5. Remove the wheelhouse brace trim.
6. Remove the bolts and the rear seat back cushion latch striker.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat back cushion latch striker with the bolts.

Tighten
Tighten the rear seat back cushion latch striker bolts to 24 N·m (18 lb ft).

2. Install the wheelhouse brace trim.
3. Install the front wheelhouse trim.
4. Install the rear rocker panel cover.
5. Install the rear seat back. Refer to Rear Split Folding Seat Back Replacement .
6. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .