For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
001 | Driver Air Bag Deployment Loop Resistance Too High | SDM | DTC 001 in SIR
002 | Driver Air Bag Deployment Loop Resistance Too Low | SDM | DTC 002 in SIR
003 | Driver Air Bag Deployment Loop Short to Ground | SDM | DTC 003 in SIR
004 | Driver Air Bag Deployment Loop Short to Voltage | SDM | DTC 004 in SIR
005 | Passenger Air Bag Deployment Loop Resistance Too High | SDM | DTC 005 in SIR
006 | Passenger Air Bag Deployment Loop Resistance Too Low | SDM | DTC 006 in SIR
007 | Passenger Air Bag Deployment Loop Short to Ground | SDM | DTC 007 in SIR
008 | Passenger Air Bag Deployment Loop Short to Voltage | SDM | DTC 008 in SIR
009 | Driver Pretensioner Deployment Loop Resistance Too High | SDM | DTC 009 in SIR
010 | Driver Pretensioner Deployment Loop Resistance Too Low | SDM | DTC 010 in SIR
011 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC 011 in SIR
012 | Driver Pretensioner Deployment Loop Short to Voltage | SDM | DTC 012 in SIR
013 | Passenger Pretensioner Deployment Loop Resistance Too High | SDM | DTC 013 in SIR
014 | Passenger Pretensioner Deployment Loop Resistance Too Low | SDM | DTC 014 in SIR
015 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC 015 in SIR
016 | Passenger Pretensioner Deployment Loop Short to Voltage | SDM | DTC 016 in SIR
023 | Battery Voltage High | SDM | DTC 023 in SIR
024 | Battery Voltage Low | SDM | DTC 024 in SIR
025 | SIR Warning Lamp | SDM | DTC 025 in SIR
031 | SDM Not Reusable | SDM | DTC 031 in SIR
032 | Crash Frontal Recorded | SDM | DTC 032 in SIR
033 | LH Side Air Bag Deployment Commanded | SDM | DTC 033 in SIR
034 | RH Side Air Bag Deployment Commanded | SDM | DTC 034 in SIR
035 | Pretensioner Only Deployment Commanded | SDM | DTC 035 in SIR
052 | Left Side Air Bag Deployment Loop Resistance Too High | SDM | DTC 052 in SIR
053 | Left Side Air Bag Deployment Loop Resistance Too Low | SDM | DTC 053 in SIR
054 | Left Side Air Bag Deployment Loop Short to Ground | SDM | DTC 054 in SIR
055 | Left Side Air Bag Deployment Loop Short to Voltage | SDM | DTC 055 in SIR
056 | Right Side Air Bag Deployment Loop Resistance Too High | SDM | DTC 056 in SIR
057 | Right Side Air Bag Deployment Loop Resistance Too Low | SDM | DTC 057 in SIR
058 | Right Side Air Bag Deployment Loop Short to Ground | SDM | DTC 058 in SIR
059 | Right Side Air Bag Deployment Loop Short to Voltage | SDM | DTC 059 in SIR
080 | LH Side Impact Sensor Short to Voltage or Circuit Open | SDM | DTC 080 in SIR
081 | LH Side Impact Sensor Short to Ground | SDM | DTC 081 in SIR
082 | LH Side Impact Sensor Communication Invalid | SDM | DTC 082 in SIR
083 | Left Side Impact Sensor (SIS) Initialization Status | SDM | DTC 083 in SIR
084 | RH Side Impact Sensor Short to Voltage or Circuit Open | SDM | DTC 084 in SIR
085 | RH Side Impact Sensor Short to Ground | SDM | DTC 085 in SIR
086 | RH Side Impact Sensor Communication Invalid | SDM | DTC 086 in SIR
087 | Right Side Impact Sensor (SIS) Initialization Status | SDM | DTC 087 in SIR
B1101 | Battery Voltage High | SDM | DTC B1101 in SIR
B1102 | Battery Voltage Low | SDM | DTC B1102 in SIR
B1103 | SIR Serial Communications Fault | SDM | DTC B1103 in SIR
B1104 | Passenger Seat Occupant Classification System (OCS) Voltage Out of Range | SDM | DTC B1104 in SIR
B1326 | Front End Sensor 1 Short to Ground | SDM | DTC B1326 in SIR
B1327 | Passenger Air Bag Disabled Indicator Circuit Low | SDM | DTC B1327 in SIR
B1328 | Front End Sensor 1 Internal Electronic Failure | SDM | DTC B1328 in SIR
B1329 | Front End Sensor 1 Invalid Serial Data Received | SDM | DTC B1329 in SIR
B1330 | Incorrect Electronic Front End Sensor 1 Installed | SDM | DTC B1330 in SIR
B1331 | LF Side Deployment Loop Short to Ground | SDM | DTC B1331 in SIR
B1332 | Front End Sensor 2 Short to Battery | SDM | DTC B1332 in SIR
B1333 | RF Side Deployment Loop Open | SDM | DTC B1333 in SIR
B1334 | RF Side Deployment Loop Resistance Low | SDM | DTC B1334 in SIR
B1335 | RF Side Deployment Loop Short to Ground | SDM | DTC B1335 in SIR
B1346 | Driver Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1346 in SIR
B1347 | Driver Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1347 in SIR
B1348 | Driver Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1348 in SIR
B1349 | Driver Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1349 in SIR
B1352 | Passenger Frontal Deployment Loop Stage 1 Resistance Below Threshold | SDM | DTC B1352 in SIR
B1353 | Passenger Frontal Deployment Loop Stage 1 Resistance Above Threshold | SDM | DTC B1353 in SIR
B1354 | Passenger Frontal Deployment Loop Stage 1 Short to Ground | SDM | DTC B1354 in SIR
B1355 | Passenger Frontal Deployment Loop Stage 1 Short to Battery | SDM | DTC B1355 in SIR
B1361 | Driver Pretensioner Deployment Loop Resistance High | SDM | DTC B1361 in SIR
B1362 | Driver Pretensioner Deployment Loop Resistance Low | SDM | DTC B1362 in SIR
B1363 | Driver Pretensioner Deployment Loop Short to Ground | SDM | DTC B1363 in SIR
B1364 | Driver Pretensioner Deployment Loop Short to Battery | SDM | DTC B1364 in SIR
B1367 | Passenger Pretensioner Deployment Loop Resistance High | SDM | DTC B1367 in SIR
B1368 | Passenger Pretensioner Deployment Loop Resistance Low | SDM | DTC B1368 in SIR
B1369 | Passenger Pretensioner Deployment Loop Short to Ground | SDM | DTC B1369 in SIR
B1370 | Passenger Pretensioner Deployment Loop Short to Battery | SDM | DTC B1370 in SIR
B1378 | LF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1378 in SIR
B1379 | LF Side Deployment Loop Resistance Low | SDM | DTC B1379 in SIR
B1380 | LF Side Deployment Loop Short to Ground | SDM | DTC B1380 in SIR
B1381 | LF Side Deployment Loop Short to Battery | SDM | DTC B1381 in SIR
B1382 | RF Side Deployment Loop Resistance Above Threshold | SDM | DTC B1382 in SIR
B1383 | RF Side Deployment Loop Resistance Low | SDM | DTC B1383 in SIR
B1384 | RF Side Deployment Loop Short to Ground | SDM | DTC B1384 in SIR
B1385 | RF Side Deployment Loop Short to Battery | SDM | DTC B1385 in SIR
B1395 | Deployment Loops Interconnect Circuit | SDM | DTC B1395 in SIR
B1400 | Driver SIS Malfunction | SDM | DTC B1400 in SIR
B1401 | LF Side Impact Sensor Short to Ground | SDM | DTC B1401 in SIR
B1402 | LF Side Impact Sensor Short to Battery | SDM | DTC B1402 in SIR
B1403 | Passenger SIS Malfunction | SDM | DTC B1403 in SIR
B1404 | RF Side Impact Sensor Short to Ground | SDM | DTC B1404 in SIR
B1405 | RF Side Impact Sensor Short to Battery | SDM | DTC B1405 in SIR
B1409 | LF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1409 in SIR
B1410 | RF Side Impact Sensor Invalid Serial Data Received | SDM | DTC B1410 in SIR
B1414 | LF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1414 in SIR
B1415 | RF Side Impact Sensor Incorrect Component Installed | SDM | DTC B1415 in SIR
B1440 | Passenger Seat Occupant Classification System (OCS) Circuit Short to Ground | SDM | DTC B1440 in SIR
B1446 | Passenger Seat Occupant Classification System (OCS) Circuit Short to Battery | SDM | DTC B1446 in SIR
B1447 | Passenger Seat Occupant Classification System (OCS) Sensor Circuit | SDM | DTC B1447 in SIR
B1448 | Passenger Seat Occupant Classification System (OCS) Sensor | SDM | DTC B1448 in SIR
B1449 | Passenger Seat Occupant Classification Sensor Communication | SDM | DTC B1449 in SIR
B1450 | Incorrect Passenger Seat Occupant Classification Sensor Installed | SDM | DTC B1450 in SIR
B1481 | Driver Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1481 in SIR
B1482 | Driver Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1482 in SIR
B1483 | Driver Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1483 in SIR
B1484 | Driver Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1484 in SIR
B1485 | Passenger Frontal Deployment Loop Stage 2 Resistance Above Threshold | SDM | DTC B1485 in SIR
B1486 | Passenger Frontal Deployment Loop Stage 2 Resistance Below Threshold | SDM | DTC B1486 in SIR
B1487 | Passenger Frontal Deployment Loop Stage 2 Short to Ground | SDM | DTC B1487 in SIR
B1488 | Passenger Frontal Deployment Loop Stage 2 Short to Battery | SDM | DTC B1488 in SIR
B1620 | ECU Performance | SDM | DTC B1620 in SIR
B1650 | Frontal Stage 1 Deployment Commanded | SDM | DTC B1650 in SIR
B1651 | LH Side Air Bag Deployment Commanded | SDM | DTC B1651 in SIR
B1652 | RH Side Air Bag Deployment Commanded | SDM | DTC B1652 in SIR
B1657 | Deployment Commanded Pretensioner | SDM | DTC B1657 in SIR
B1670 | Frontal Stage 2 Deployment Commanded | SDM | DTC B1670 in SIR
B2500 | Inflatable Restraint System Indicator Circuit | SDM | DTC B2500 in SIR
B2502 | Passenger Air Bag Disabled Indicator Circuit Malfunction | SDM | DTC B2502 in SIR
C1101 | Battery Voltage High | EBCM | DTC C1101 in Antilock Brake System
C1102 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1102 in Antilock Brake System
C1200 | Left Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1200 in Antilock Brake System
C1201 | Left Front Wheel Speed Circuit Range Performance | EBCM | DTC C1201 in Antilock Brake System
C1202 | Left Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1202 in Antilock Brake System
C1203 | Right Front Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1203 in Antilock Brake System
C1204 | Right Front Wheel Speed Circuit Range Performance | EBCM | DTC C1204 in Antilock Brake System
C1205 | Right Front Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1205 in Antilock Brake System
C1206 | Left Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1206 in Antilock Brake System
C1207 | Left Rear Wheel Speed Sensor Circuit Range Performance | EBCM | DTC C1207 in Antilock Brake System
C1208 | Left Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1208 in Antilock Brake System
C1209 | Right Rear Wheel Speed Sensor Circuit Open or Shorted | EBCM | DTC C1209 in Antilock Brake System
C1210 | ECU Malfunction | EBCM | DTC C1210 in Antilock Brake System
C1211 | Right Rear Wheel Speed Sensor Input Signal Equals Zero | EBCM | DTC C1211 in Antilock Brake System
C1604 | ECU Malfunction | EBCM | DTC C1604 in Antilock Brake System
C2112 | Solenoid Valve Relay Circuit | EBCM | DTC C2112 in Antilock Brake System
C2402 | Pump Motor Circuit | EBCM | DTC C2402 in Antilock Brake System
P0016 | Camshaft Position (CMP) Sensor Performance | ECM | DTC P0016 or P0340 for the 1.6L engine (L91)
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030 or P0036 for the 1.2L engine
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.6L engine (L91)
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.6L engine (L91)
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0030 or P0036 for the 1.2L engine
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.6L engine (L91)
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0031, P0032, P0037, or P0038 for the 1.6L engine (L91)
P0068 | Throttle Body Air Flow Performance | ECM | DTC P0068 for the 1.6L engine (L91)
P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM |

• | DTC P0106 for the 1.4L DOHC engine

• | DTC P0106 for the 1.4L SOHC engine

• | DTC P0106 for the 1.6L engine (L91)

P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2L engine

• | DTC P0107 or P0108 for the 1.4L DOHC engine

• | DTC P0107 or P0108 for the 1.4L SOHC engine

• | DTC P0107 or P0108 for the 1.5L engine

• | DTC P0107 or P0108 for the 1.6L engine (L91)

P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM |

• | DTC P0107 or P0108 for the 1.2L engine

• | DTC P0107 or P0108 for the 1.4L DOHC engine

• | DTC P0107 or P0108 for the 1.4L SOHC engine

• | DTC P0107 or P0108 for the 1.5L engine

• | DTC P0107 or P0108 for the 1.6L engine (L91)

P0110 | Intake Air Temperature (IAT) Sensor Circuit | ECM | DTC P0110 or P0111 for the 1.6L engine (L91)
P0111 | Intake Air Temperature (IAT) Sensor Performance | ECM | DTC P0110 or P0111 for the 1.6L engine (L91)
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2L engine

• | DTC P0112 or P0113 for the 1.4L DOHC engine

• | DTC P0112 or P0113 for the 1.4L SOHC engine

• | DTC P0112 or P0113 for the 1.5L engine

• | DTC P0112 or P0113 for the 1.6L engine (L91)

P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM |

• | DTC P0112 or P0113 for the 1.2L engine

• | DTC P0112 or P0113 for the 1.4L DOHC engine

• | DTC P0112 or P0113 for the 1.4L SOHC engine

• | DTC P0112 or P0113 for the 1.5L engine

• | DTC P0112 or P0113 for the 1.6L engine (L91)

P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116 for the 1.6L engine (L91)
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2L engine

• | DTC P0117 or P0118 for the 1.4L DOHC engine

• | DTC P0117 or P0118 for the 1.4L SOHC engine

• | DTC P0117 or P0118 for the 1.5L engine

• | DTC P0117 or P0118 for the 1.6L engine (L91)

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM |

• | DTC P0117 or P0118 for the 1.2L engine

• | DTC P0117 or P0118 for the 1.4L DOHC engine

• | DTC P0117 or P0118 for the 1.4L SOHC engine

• | DTC P0117 or P0118 for the 1.6L engine (L91)

P0117 or P0118 | Engine Coolant Temperature (ECT) Sensor Circuit Low or High Voltage | ECM | DTC P0117 or P0118 for the 1.5L engine
P0122 | Throttle Position (TP) Sensor Circuit Low Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine

• | DTC P0122 or P0123 for the 1.4L DOHC engine

• | DTC P0122 or P0123 for the 1.4L SOHC engine

• | DTC P0122 or P0123 for the 1.5L engine

P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine (L91)
P0123 | Throttle Position (TP) Sensor Circuit High Voltage | ECM |

• | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine

• | DTC P0122 or P0123 for the 1.4L DOHC engine

• | DTC P0122 or P0123 for the 1.4L SOHC engine

• | DTC P0122 or P0123 for the 1.5L engine

• | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine (L91)

P0125 | Engine Coolant Temperature (ECT) Insufficient for Close Loop | ECM | DTC P0125 or P0128 for the 1.6L engine (L91)
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM | DTC P0125 or P0128 for the 1.6L engine (L91)
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM |

• | DTC P0131 or P0137 for the 1.2L engine

• | DTC P0131 or P0132 for the 1.4L DOHC engine

• | DTC P0131 or P0132 for the 1.4L SOHC engine

• | DTC P0131 or P0132 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine (L91)

P0132 | HO2S Circuit High Voltage Sensor 1 | ECM |

• | DTC P0132 or P0138 for the 1.2L engine

• | DTC P0131 or P0132 for the 1.4L DOHC engine

• | DTC P0131 or P0132 for the 1.4L SOHC engine

• | DTC P0131 or P0132 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine (L91)

P0133 | HO2S Slow Response Sensor 1 | ECM |

• | DTC P0133 for the 1.2L engine

• | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine

• | DTC P0133, P1133, or P1134 for the 1.4L SOHC engine

• | DTC P0133 or P0139 for the 1.6L engine (L91)

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM |

• | DTC P0134 or P0140 for the 1.4L DOHC engine

• | DTC P0134 or P0140 for the 1.4L SOHC engine

• | DTC P0134 for the 1.5L engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine (L91)

P0135 | HO2S Heater Performance Sensor 1 | ECM |

• | DTC P0135 or P0141 for the 1.2L engine

• | DTC P0135 or P0141 for the 1.4L DOHC engine

• | DTC P0135 or P0141 for the 1.4L SOHC engine

• | DTC P0135 or P0141 for the 1.6L engine (L91)

P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM |

• | DTC P0131 or P0137 for the 1.2L engine

• | DTC P0137 or P0138 for the 1.4L DOHC engine

• | DTC P0137 or P0138 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine (L91)

P0138 | HO2S Circuit High Voltage Sensor 2 | ECM |

• | DTC P0132 or P0138 for the 1.2L engine

• | DTC P0137 or P0138 for the 1.4L DOHC engine

• | DTC P0137 or P0138 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine (L91)

P0139 | HO2S Slow Response Sensor 2 | ECM | DTC P0133 or P0139 for the 1.6L engine (L91)
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM |

• | DTC P0140 for the 1.2L engine

• | DTC P0134 or P0140 for the 1.4L DOHC engine

• | DTC P0134 or P0140 for the 1.4L SOHC engine

• | DTC P0131, P0132, P0134, P0137, P0138, or P0140 for the 1.6L engine (L91)

P0141 | HO2S Heater Performance Sensor 2 | ECM |

• | DTC P0135 or P0141 for the 1.2L engine

• | DTC P0135 or P0141 for the 1.4L DOHC engine

• | DTC P0135 or P0141 for the 1.4L SOHC engine

• | DTC P0135 or P0141 for the 1.6L engine (L91)

P0171 | Fuel Trim System Lean | ECM |

• | DTC P0171 or P0172 for the 1.2L engine

• | DTC P0171 or P0172 for the 1.4L DOHC engine

• | DTC P0171 or P0172 for the 1.4L SOHC engine

• | DTC P0171, P0172, P2187, or P2188 for the 1.6L engine (L91)

P0172 | Fuel Trim System Rich | ECM |

• | DTC P0171 or P0172 for the 1.2L engine

• | DTC P0171 or P0172 for the 1.4L DOHC engine

• | DTC P0171 or P0172 for the 1.4L SOHC engine

• | DTC P0171, P0172, P2187, or P2188 for the 1.6L engine (L91)

P0201 | Injector 1 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0202 | Injector 2 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0203 | Injector 3 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0204 | Injector 4 Control Circuit | ECM |

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L DOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.4L SOHC engine

• | DTC P0201, P0202, P0203, or P0204 for the 1.5L engine

P0217 | Engine Coolant Over Temperature | ECM | DTC P0217 for the 1.6L engine (L91)
P0222 | Idle Speed Control (ISP) Motor Position Sensor Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine (L91)
P0223 | Idle Speed Control (ISP) Motor Position Sensor Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223 for the 1.2L engine
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine (L91)
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.2L engine or DTC P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine (L91)
P0300 | Engine Misfire Detected | ECM |

• | DTC P0300 for the 1.2L engine

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine (L91)

P0301 | Cylinder 1 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine (L91)

P0302 | Cylinder 2 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine (L91)

P0303 | Cylinder 3 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine (L91)

P0304 | Cylinder 4 Misfire Detected | ECM |

• | DTC P0300-P0304 for the 1.4L DOHC engine

• | DTC P0300-P0304 for the 1.4L SOHC engine

• | DTC P0300-P0304 for the 1.6L engine (L91)

P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P0315 for the 1.6L engine (L91)
P0317 | Rough Road Sensing System Input Not Present | ECM | DTC P0317 for the 1.4L DOHC engine or DTC P0317 for the 1.4L SOHC engine
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324 for the 1.4L DOHC engine or DTC P0324 for the 1.6L engine (L91)
P0325 | Knock Sensor (KS) Circuit | ECM |

• | DTC P0325 for the 1.4L DOHC engine

• | DTC P0325 for the 1.4L SOHC engine

• | DTC P0325 for the 1.5L engine

• | DTC P0325 for the 1.6L engine (L91)

P0327 | Knock Sensor (KS) Circuit | ECM | DTC P0327 for the 1.2L engine or DTC P0327 for the 1.5L engine
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0335, P0336, or P0337 for the 1.4L DOHC engine

• | DTC P0335 or P0336 for the 1.6L engine (L91)

P0336 | Crankshaft Position (CKP) Sensor Performance | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0335, P0336, or P0337 for the 1.4L DOHC engine

• | DTC P0336 or P0337 for the 1.4L SOHC engine

• | DTC P0336 or P0337 for the 1.5L engine

• | DTC P0335 or P0336 for the 1.6L engine (L91)

P0337 | Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle | ECM |

• | DTC P0335, P0336, or P0337 for the 1.2L engine

• | DTC P0336 or P0337 for the 1.4L SOHC engine

• | DTC P0336 or P0337 for the 1.5L engine

P0340 | Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0016 or P0340 for the 1.6L engine (L91)
P0341 | Camshaft Position (CMP) Sensor Performance | ECM |

• | DTC P0341 or P0342 for the 1.2L engine

• | DTC P0341 or P0342 for the 1.4L SOHC engine

• | DTC P0341 or P0342 for the 1.5L engine

P0342 | Camshaft Position (CMP) Sensor Circuit Low Voltage | ECM |

• | DTC P0341 or P0342 for the 1.2L engine

• | DTC P0341 or P0342 for the 1.4L SOHC engine

• | DTC P0341 or P0342 for the 1.5L engine

P0351 | Ignition Coil 1 and 4 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2L engine

• | DTC P0351 or P0352 for the 1.4L DOHC engine

• | DTC P0351 or P0352 for the 1.4L SOHC engine

• | DTC P0351 or P0352 for the 1.5L engine

• | DTC P0351 or P0352 for the 1.6L engine (L91)

P0352 | Ignition Coil 2 Control Circuit | ECM |

• | DTC P0351 or P0352 for the 1.2L engine

• | DTC P0351 or P0352 for the 1.4L DOHC engine

• | DTC P0351 or P0352 for the 1.4L SOHC engine

• | DTC P0351 or P0352 for the 1.5L engine

• | DTC P0351 or P0352 for the 1.6L engine (L91)

P0400 | Exhaust Gas Recirculation (EGR) Flow Incorrect | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine (L91)

P0401 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine (L91)

P0402 | Exhaust Gas Recirculation (EGR) Flow Excessive | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine (L91)

P0403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine
P0404 | Exhaust Gas Recirculation (EGR) Open Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine (L91)

P0405 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine (L91)

P0406 | Exhaust Gas Recirculation (EGR) Position Sensor Circuit High Voltage | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

• | DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine (L91)

P0420 | Catalyst System Low Efficiency | ECM |

• | DTC P0420 for the 1.2L engine

• | DTC P0420 for the 1.4L DOHC engine

• | DTC P0420 for the 1.4L SOHC engine

• | DTC P0420 for the 1.6L engine (L91)

P042E | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine or DTC P0403, P0404, P0405, P0406, or P042E for the 1.6L engine (L91)
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442 or P0456 for the 1.6L engine (L91)
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM |

• | DTC P0443 for the 1.4L DOHC engine

• | DTC P0443 for the 1.4L SOHC engine

• | DTC P0443 for the 1.5L engine

P0444 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0444 or P0445 for the 1.2L engine
P0445 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0444 or P0445 for the 1.2L engine
P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM | DTC P0446 for the 1.6L engine (L91)
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0451 or P0454 for the 1.6L engine (L91)
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453 for the 1.6L engine (L91)
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453 for the 1.6L engine (L91)
P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM | DTC P0451 or P0454 for the 1.6L engine (L91)
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455 for the 1.6L engine (L91)
P0456 | Evaporative Emission (EVAP) System Very Small Leak Detected | ECM | DTC P0442 or P0456 for the 1.6L engine (L91)
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Open | ECM | DTC P0458 or P0459 for the 1.6L engine (L91)
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Shorted | ECM | DTC P0458 or P0459 for the 1.6L engine (L91)
P0496 | Evaporative Emission (EVAP) System Continuous Purge Flow | ECM | DTC P0496 for the 1.6L engine (L91)
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Open | ECM | DTC P0498 or P0499 for the 1.6L engine (L91)
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Shorted | ECM | DTC P0498 or P0499 for the 1.6L engine (L91)
P0501 | Vehicle Speed Sensor (VSS) Circuit | ECM | DTC P0501 for the 1.2L engine
P0502 | Vehicle Speed Sensor (VSS) Circuit | ECM |

• | DTC P0502 for the 1.4L DOHC engine

• | DTC P0502 for the 1.4L SOHC engine

• | DTC P0502 for the 1.5L engine

• | DTC P0502 for the 1.6L engine (L91)

P0504 | Brake Switch 1-2 Corrilation | ECM | DTC P0504
P0506 | Idle Speed Low | ECM |

• | DTC P0506 or P0507 for the 1.4L DOHC engine

• | DTC P0506 or P0507 for the 1.4L SOHC engine

• | DTC P0506 or P0507 for the 1.6L engine (L91)

P0507 | Idle Speed High | ECM |

• | DTC P0506 or P0507 for the 1.4L DOHC engine

• | DTC P0506 or P0507 for the 1.4L SOHC engine

• | DTC P0506 or P0507 for the 1.6L engine (L91)

P0510 | Idle Position Switch Circuit | ECM | DTC P0510 for the 1.2L engine
P0562 | System Voltage Low | TCM | DTC P0562 in Automatic Transaxle - Aisin (81-40LE)
P0563 | System Voltage High | TCM | DTC P0563 in Automatic Transaxle - Aisin (81-40LE)
P0600 | Control Module Internal Performance | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P0601 | Control Module Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601 or P1790 in Automatic Transaxle - Aisin (81-40LE)
P0602 | Control Module Not Programmed | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

P0603 | Control Module Long Term Memory Reset | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

P0604 | Control Module Random Access Memory (RAM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

TCM | DTC P0604 in Automatic Transaxle - Aisin (81-40LE)
P0605 | Control Module Programming Read Only Memory (ROM) | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

P0606 | Control Module Internal Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

P0607 | Control Module Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

P061B | Control Module Internal Performance | ECM | DTC P061B or P161B for the 1.6L engine (L91)
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629 for the 1.2L engine
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629 for the 1.2L engine
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641 or P0651 for the 1.6L (L91) engine
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650 or P1650 for the 1.2L engine or DTC P0650 for the 1.6L (L91) engine
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641 or P0651 for the 1.6L engine (L91)
P0660 | Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit | ECM | DTC P0660 for the 1.4L DOHC engine or DTC P0660 for the 1.6L (L91) engine
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685 for the 1.6L (L91) engine
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM |

• | DTC P0700 for the 1.4L DOHC engine

• | DTC P0700 for the 1.4L SOHC engine

• | DTC P0700 for the 1.6L (L91) engine

P0705 | Transmission Range Sensor Circuit | TCM | DTC P0705 in Automatic Transaxle - Aisin (81-40LE)
P0706 | Transmission Range (TR) Switch Performance | TCM | DTC P0706 in Automatic Transaxle - Aisin (81-40LE)
P0711 | Transmission Fluid Temperature Sensor (TFT) Sensor Performance | TCM | DTC P0711 in Automatic Transaxle - Aisin (81-40LE)
P0712 | Transmission Fluid Temperature Sensor Low Input | TCM | DTC P0712 in Automatic Transaxle - Aisin (81-40LE)
P0713 | Transmission Fluid Temperature Sensor Circuit High input | TCM | DTC P0713 in Automatic Transaxle - Aisin (81-40LE)
P0717 | Input Speed Sensor - No Signal | TCM | DTC P0717 in Automatic Transaxle - Aisin (81-40LE)
P0722 | Output Speed Sensor Circuit No Signal | TCM | DTC P0722 in Automatic Transaxle - Aisin (81-40LE)
P0727 | Engine Speed Signal Circuit | TCM | DTC P0727 in Automatic Transaxle - Aisin (81-40LE)
P0741 | Torque Converter Clutch (TCC) System-Stuck Off | TCM | DTC P0741 in Automatic Transaxle - Aisin (81-40LE)
P0742 | Torque Converter Clutch Circuit Stuck On | TCM | DTC P0742 in Automatic Transaxle - Aisin (81-40LE)
P0743 | Torque Converter Clutch Circuit Electrical | TCM | DTC P0743 in Automatic Transaxle - Aisin (81-40LE)
P0748 | Pressure Control Solenoid Electrical | TCM | DTC P0748 in Automatic Transaxle - Aisin (81-40LE)
P0751 | Shift Solenoid 1 Performance or Stuck Off | TCM | DTC P0751 in Automatic Transaxle - Aisin (81-40LE)
P0752 | Shift Solenoid 1 Performance Stuck On | TCM | DTC P0752 in Automatic Transaxle - Aisin (81-40LE)
P0753 | Shift Solenoid 1 Electrical | TCM | DTC P0753 in Automatic Transaxle - Aisin (81-40LE)
P0756 | Shift Solenoid 2 Performance or Stuck Off | TCM | DTC P0756 in Automatic Transaxle - Aisin (81-40LE)
P0757 | Shift Solenoid (SS) 2 Performance Stuck On | TCM | DTC P0757 in Automatic Transaxle - Aisin (81-40LE)
P0758 | Shift Solenoid 2 Electrical | TCM | DTC P0758 in Automatic Transaxle - Aisin (81-40LE)
P0785 | Shift Timing Solenoid | TCM | DTC P0785 or P1710 in Automatic Transaxle - Aisin (81-40LE)
P0787 | Shift Timing Solenoid Low Voltage | TCM | DTC P0787 in Automatic Transaxle - Aisin (81-40LE)
P0788 | Shift Timing Solenoid High Voltage | TCM | DTC P0788 in Automatic Transaxle - Aisin (81-40LE)
P0834 | Clutch Pedal Switch Circuit Low Voltage | ECM | DTC P0834
P0835 | Clutch Pedal Switch Circuit High Voltage | ECM | DTC P0835
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0962 in Automatic Transaxle - Aisin (81-40LE)
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0963 in Automatic Transaxle - Aisin (81-40LE)
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973 in Automatic Transaxle - Aisin (81-40LE)
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0974 in Automatic Transaxle - Aisin (81-40LE)
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976 in Automatic Transaxle - Aisin (81-40LE)
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0977 in Automatic Transaxle - Aisin (81-40LE)
P1106 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4L DOHC engine

• | DTC P1106 or P1107 for the 1.4L SOHC engine

• | DTC P1106 or P1107 for the 1.5L engine

P1107 | Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1106 or P1107 for the 1.4L DOHC engine

• | DTC P1106 or P1107 for the 1.4L SOHC engine

• | DTC P1106 or P1107 for the 1.5L engine

P1111 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4L DOHC engine

• | DTC P1111 or P1112 for the 1.4L SOHC engine

• | DTC P1111 or P1112 for the 1.5L engine

P1112 | Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1111 or P1112 for the 1.4L DOHC engine

• | DTC P1111 or P1112 for the 1.4L SOHC engine

• | DTC P1111 or P1112 for the 1.5L engine

P1114 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4L DOHC engine

• | DTC P1114 or P1115 for the 1.4L SOHC engine

• | DTC P1114 or P1115 for the 1.5L engine

P1115 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage | ECM |

• | DTC P1114 or P1115 for the 1.4L DOHC engine

• | DTC P1114 or P1115 for the 1.4L SOHC engine

• | DTC P1114 or P1115 for the 1.5L engine

P1121 | Throttle Position (TP) Sensor Circuit Intermittent High Voltage | P1121 |

• | DTC P1121 or P1122 for the 1.4L DOHC engine

• | DTC P1121 or P1122 for the 1.4L SOHC engine

• | DTC P1121 or P1122 for the 1.5L engine

P1122 | Throttle Position (TP) Sensor Circuit Intermittent Low Voltage | ECM |

• | DTC P1121 or P1122 for the 1.4L DOHC engine

• | DTC P1121 or P1122 for the 1.4L SOHC engine

• | DTC P1121 or P1122 for the 1.5L engine

P1133 | HO2S Insufficient Switching Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine or DTC P0133, P1133, or P1134 for the 1.4L SOHC engine
P1134 | HO2S Transition Time Ratio Sensor 1 | ECM | DTC P0133, P1133, or P1134 for the 1.4L DOHC engine or DTC P0133, P1133, or P1134 for the 1.4L SOHC engine
P1137 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1137 or P1166 for the 1.6L (L91) engine
P1138 | HO2S Circuit High Voltage During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1138 or P2297 for the 1.6L (L91) engine
P1166 | HO2S Circuit Low Voltage During Power Enrichment Sensor 2 | ECM | DTC P1166 for the 1.4L DOHC engine or DTC P1137 or P1166 for the 1.6L (L91) engine
P1167 | HO2S Circuit High Voltage During Decel Fuel Cut-Off (DFCO) Sensor 1 | ECM | DTC P1167 for the 1.4L DOHC engine or DTC P1167 for the 1.4L SOHC engine
P1171 | HO2S Circuit Low Voltage During Power Enrichment Sensor 1 | ECM | DTC P1171 for the 1.4L DOHC engine or DTC P1171 for the 1.4L SOHC engine
P1230 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P1230 or P1231 for the 1.2L engine
P1231 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P1230 or P1231 for the 1.2L engine
P1320 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1320 for the 1.2L engine
P1321 | Crankshaft Position (CKP) Reluctor Wheel Performance | ECM | DTC P1321 for the 1.2L engine
P1336 | Crankshaft Position (CKP) System Variation Not Learned | ECM | DTC P1336 for the 1.4L DOHC engine or DTC P1336 for the 1.4L SOHC engine
P1380 | Misfire Detected - Rough Road Data Not Available | ECM | DTC P1380 or P1381 for the 1.4L DOHC engine
P1381 | Misfire Detected - No Communication With Brake Control Module | ECM | DTC P1380 or P1381 for the 1.4L DOHC engine or DTC P1380 or P1381 for the 1.4L SOHC engine
P1382 | Wheel Speed Sensor Circuit Performance | ECM | DTC P1382 or P1385 for the 1.2L engine
P1385 | Wheel Speed Sensor Circuit | ECM | DTC P1382 or P1385 for the 1.2L engine
P1390 | Left Driven Wheel Speed Sensor Circuit | ECM | DTC P1390 or P1396 for the 1.2L engine
P1391 | Rough Road Sensor Performance | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L (L91) engine

P1392 | Rough Road Sensor Circuit Low Voltage | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L (L91) engine

P1393 | Rough Road Sensor Circuit High Voltage | ECM |

• | DTC P1391, P1392, or P1393 for the 1.4L DOHC engine

• | DTC P1391, P1392, or P1393 for the 1.4L SOHC engine

• | DTC P1391, P1392, or P1393 for the 1.6L (L91) engine

P1396 | Wheel Speed Sensor Circuit w/o ABS | ECM |

• | DTC P1390 or P1396 for the 1.2L engine

• | DTC P1396 or P1397 for the 1.4L DOHC engine

• | DTC P1396 or P1397 for the 1.6L (L91) engine

P1397 | Wheel Speed Sensor Circuit w/ABS | ECM | DTC P1396 or P1397 for the 1.4L DOHC engine or DTC P1396 or P1397 for the 1.6L (L91) engine
P1402 | Exhaust Gas Recirculation (EGR) Flow Insufficient | ECM |

• | DTC P0400, P0401, P0402, or P1402 for the 1.2L engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L DOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.4L SOHC engine

• | DTC P0400, P0401, P0402, or P1402 for the 1.6L engine (L91)

P1403 | Exhaust Gas Recirculation (EGR) Solenoid Control Circuit | ECM | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine
P1404 | Exhaust Gas Recirculation (EGR) Closed Position Performance | ECM |

• | DTC P0403, P0404, P0405, P0406, P1403, or P1404 for the 1.2L engine

• | DTC P0404-P0406, P042E, or P1404 for the 1.4L DOHC engine

• | DTC P0404, P0405, P0406, or P1404 for the 1.4L SOHC engine

P1504 | Vehicle Speed Output Circuit 2 | ECM | DTC P1504 for the 1.2L engine
P1511 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P1511, P1512, or P1513 for the 1.2L engine
P1512 | Idle Speed Control (ISC) System | ECM | DTC P1511, P1512, or P1513 for the 1.2L engine
P1513 | Idle Speed Control (ISC) System Performance | ECM | DTC P1511, P1512, or P1513 for the 1.2L engine
P1516 | Throttle Actuator control (TAC) Module Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119 for the 1.6L (L91) engine
P1601 | Lost Communication with TCM | ECM |

• | DTC P1601 for the 1.4L DOHC engine

• | DTC P1601 for the 1.4L SOHC engine

• | DTC P1601 for the 1.5L engine

P1607 | -- | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P1610 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P1610 or P1611 for the 1.2L engine
P1611 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P1610 or P1611 for the 1.2L engine
P161B | Control Module Torque Performance | ECM | DTC P061B or P161B for the 1.6L engine (L91)
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1650 or P1651 for the 1.2L engine
P1650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM |

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

P1651 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1650 or P1651 for the 1.2L engine
P1660 | Malfunction Indicator Lamp (MIL) Control Circuit High Voltage | ECM | DTC P1660 or P1661 for the 1.2L engine
P1661 | Malfunction Indicator Lamp (MIL) Control Circuit Low Voltage | ECM | DTC P1660 or P1661 for the 1.2L engine
P1701 | Engine Coolant Temperature (ECT) Sensor Circuit | TCM | DTC P1701 or P1792 in Automatic Transaxle - Aisin (81-40LE)
P1702 | Engine Torque Signal Error | TCM | DTC P1702 in Automatic Transaxle - Aisin (81-40LE)
P1710 | Timing Solenoid Electrical | TCM | DTC P0785 or P1710 in Automatic Transaxle - Aisin (81-40LE)
P1781 | Engine Torque Signal Error | TCM | DTC P1781 in Automatic Transaxle - Aisin (81-40LE)
P1790 | Internal Control Module Memory Checksum Error | TCM | DTC P0601 or P1790 in Automatic Transaxle - Aisin (81-40LE)
P1791 | Throttle Position (TP) Sensor Circuit | TCM | DTC P1791 in Automatic Transaxle - Aisin (81-40LE)
P1792 | Engine Coolant Signal | TCM | DTC P1701 or P1792 in Automatic Transaxle - Aisin (81-40LE)
P2076 | Intake Manifold Tuning (IMT) Valve Position Sensor Performance | ECM | DTC P2076, P2077, or P2078 for the 1.6L (L91) engine
P2077 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit Low Voltage | ECM | DTC P2076, P2077, or P2078 for the 1.6L (L91) engine
P2078 | Intake Manifold Tuning (IMT) Valve Position Sensor Circuit High Voltage | ECM | DTC P2076, P2077, or P2078 for the 1.6L (L91) engine
P2101 | Idle Speed Control (ISC) Motor Control Circuit | ECM | DTC P2101, P2118, or P2119 for the 1.2L engine
P2101 | Throttle Actuator Position Performance | ECM | DTC P1516, P2101, or P2119 for the 1.6L (L91) engine
P2104 | Throttle Actuator Control (TAC) System - Forced Engine Idle | ECM | DTC P2104, P2105, P2106, or P2110 for the 1.6L (L91) engine
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2104, P2105, P2106, or P2110 for the 1.6L (L91) engine
P2106 | Throttle Control System Performance - Throttle Limitation Active | ECM | DTC P2104, P2105, P2106, or P2110 for the 1.6L (L91) engine
P2110 | Throttle Actuator Control (TAC) System - Forced Limited Engine Speed | ECM | DTC P2104, P2105, P2106, or P2110 for the 1.6L (L91) engine
P2118 | Idle Speed Control (ISC) System | ECM | DTC P2101, P2118, or P2119 for the 1.2L engine
P2119 | Idle Speed Control (ISC) System Performance | ECM | DTC P2101, P2118, or P2119 for the 1.2L engine
P2119 | Throttle Closed Position Performance | ECM | DTC P1516, P2101, or P2119 for the 1.6L (L91) engine
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6L (L91) engine
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6L (L91) engine
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6L (L91) engine
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6L (L91) engine
P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM | DTC P0122, P0123, P0222, P0223, or P2135 for the 1.6L engine (L91)
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6L (L91) engine
P2187 | Fuel Trim System Lean at Idle | ECM | DTC P0171, P0172, P2187, or P2188 for the 1.6L engine (L91)
P2188 | Fuel Trim System Rich at Idle | ECM | DTC P0171, P0172, P2187, or P2188 for the 1.6L engine (L91)
P2282 | Intake Manifold Air Leak | ECM | DTC P2282 for the 1.6L engine (L91)
P2297 | HO2S Circuit High Voltage during Decel Fuel Cut-Off (DFCO) Sensor 2 | ECM | DTC P2297 for the 1.4L DOHC engine or DTC P1138 or P2297 for the 1.6L (L91) engine
P2610 | Control Module Ignition Off Timer Performance | ECM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.2L engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L SOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.4L DOHC engine

• | DTC P0600-P0607, P1607, P1650, P1655, or P2610 for the 1.5L engine

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P1600, P1621, P1627, P1680, P1681, P1683, or P2610 for the 1.6L engine (L91)

P2769 | Torque Converter Clutch (TCC) Control Circuit Low Voltage | TCM | DTC P2769 in Automatic Transaxle - Aisin (81-40LE)
P2770 | Torque Converter Clutch (TCC) Control Circuit High Voltage | TCM | DTC P2770 in Automatic Transaxle - Aisin (81-40LE)
U0401 | Invalid Data Received from ECM/PCM | TCM | DTC U0401 in Automatic Transaxle - Aisin (81-40LE)
U2105 | CAN Bus Error | TCM | DTC U2105 in Automatic Transaxle - Aisin (81-40LE)