For 1990-2009 cars

## Door Window Regulator Replacement Manual Front

### Removal Procedure

1. Remove the front door glass. Refer to Front Side Door Window Replacement .
2. Remove the nuts and the window regulator.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the window regulator and the nuts.

Tighten
Tighten the window regulator nuts to 7 N·m (62 lb in).

2. Install the front door glass. Refer to Front Side Door Window Replacement .

## Door Window Regulator Replacement Manual Rear

### Removal Procedure

1. Remove the rear door glass. Refer to Rear Side Door Window Replacement .
2. Remove the nuts and the window regulator.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the window regulator with the nuts.

Tighten
Tighten the window regulator nuts to 7 N·m (62 lb in).

2. Install the rear door glass. Refer to Rear Side Door Window Replacement .

## Door Window Regulator Replacement Power Front

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the door glass. Refer to Front Side Door Window Replacement .
3. Remove the nuts and the regulator.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the window regulator with the nuts.

Tighten
Tighten the window regulator nuts to 7 N·m (62 lb in).

3. Install the front door glass. Refer to Front Side Door Window Replacement .
4. Connect the negative battery cable.
5. If the vehicle is equipped with a one touch up function, and the driver side power window regulator has been replaced, perform the window motor reinitialization process. Refer to Power Window Reinitialization .

## Door Window Regulator Replacement Power Rear

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear door glass. Refer to Rear Side Door Window Replacement .
3. Remove the nuts and the regulator.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the window regulator with the nuts.

Tighten
Tighten the window regulator nuts to 7 N·m (62 lb in).

3. Install the rear door glass. Refer to Rear Side Door Window Replacement .
4. Connect the negative battery cable.