For 1990-2009 cars

### Removal Procedure

1. Remove the rear seatback lock release knob.
2. Reposition the rear seatback cover.
3. Remove the screws and the lock assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seatback lock assembly with the screws.

Tighten
Tighten the rear seat back lock assembly screws to 20 N·m (15 lb ft).

2. Install the rear seatback cover to its original position.
3. Install the rear seatback lock release knob.