For 1990-2009 cars

Table 1: | General Specifications
Table 2: | Cylinder Compression Check Specifications
Table 3: | Valve Clearance Specifications

#### General Specifications

Application | Specification
--- | ---
Metric | English
Engine Information

- Engine Type

Overhead Cam L-4

- Bore

68.5 mm

2.70 in

- Compression Ratio

9.3:1

Firing Order | 1-3-4-2

- Lubricating Type

Forced Feed

- Maximum Power at 5,400 RPM

52.2 kW

71 HP

- Maximum Torque at 4,200 RPM

104 N·m

76.7 lb ft

- Oil Pump Type

Trocboid Rotor

- Oil Filter Type

Cartridge (Full Flow)

- Oil Pan Capacity Including Oil Filter

3.2 liter

3.4 quarts

- Stroke

78.0 mm

3.07 in

- Total Displacement

1150 cm³

#### Cylinder Compression Check Specifications

Condition | Cylinder Number
--- | ---
1 | 2 | 3 | 4
Compression top dead center of No. 1 cylinder

- Intake

O

O

--

--

- Exhaust

O

--

O

--

Exhaust top dead center of No. 1 cylinder

- Intake

--

--

O

O

- Exhaust

--

O

--

O

* O marks indicate the place where the valve clearance can be checked and adjusted.

#### Valve Clearance Specifications

Application | Specification
--- | ---
Metric | English
Cold

- Intake

0.15 +/- 0.02 mm

0.0059 +/- 0.0008 in

- Exhaust

0.2 +/- 0.02 mm

0.00787 +/- 0.0008 in

Hot

- Intake

0.25 +/- 0.02 mm

0.0098 +/- 0.0008 in

- Exhaust

0.3 +/- 0.02 mm

0.0118 +/- 0.0008 in

Application | Specification
--- | ---
Metric | English
Camshaft

- Bearing Outside Diameter, Head Journal I D, No. 1

43.5000-43.516 mm

1.713-1.7132 in

- Bearing Outside Diameter, Head Journal I D, No. 2

43.700-43.716 mm

1.720-1.7211 in

- Bearing Outside Diameter, Head Journal I D, No. 3

43.900-43.916 mm

1.728-1.7290 in

- Bearing Outside Diameter, Head Journal I D, No. 4

44.100-44.116 mm

1.736-1.7369 in

- Bearing Outside Diameter, Head Journal I D, No. 5

44.300-44.316 mm

1.744-1.745 in

End Play

- Journal Outside Diameter No. 1

43.425-43.450 mm

1.710-1.711 in

- Journal Outside Diameter No. 2

43.625-43.650 mm

1.718-1.719 in

- Journal Outside Diameter No. 3

43.825-43.850 mm

1.725-1.726 in

- Journal Outside Diameter No. 4

44.025-44.050 mm

1.733 1.734 in

- Journal Outside Diameter No. 5

44.225-44.250 mm

1.741-1.742 in

- Lift Exhaust

5.38 mm

0.212 in

- Lift Intake

5.42 mm

0.213 in

Crankshaft

- Connecting Rod Journal Diameter, All

37.982-38.000 mm

1.495-1.496 in

- Main Journal Crankshaft End Play

0.11-0.31 mm

0.004-0.012 in

- Main Journal Diameter, All

43.982-44.000 mm

1.7316-1.7323 in

- Main Journal Main Bearing Clearance, All

0.020-0.040 mm

0.0008-0.0016 in

- Main Journal Out of Round, Maximum

0.005 mm

0.0002 in

- Main Journal Taper, Maximum

0.005 mm

0.0002 in

- Out of Round, Maximum

0.005 mm

0.0002 in

- Rod Bearing Clearance, All

0.020-0.040 mm

0.0008-0.0016 in

- Rod Side Clearance

0.10-0.25 mm

0.004-0.010 in

- Taper, Maximum

0.005 mm

0.0002 in

Cylinder Bore

- Diameter

68.5 mm

2.70 in

- Out of Round, Maximum

0.005 mm

0.00020 in

- Taper, Maximum

0.005 mm

0.00020 in

Oil Pump

- Gap Between Oil Pump Body and Outer Rotor

0.10-0.17 mm

0.0039-0.0067 in

- Inner Rotor Side Clearance

0.065-0.115 mm

0.0026-0.0045 in

- Outer Rotor Side Clearance

0.065-0.115 mm

0.0026-0.0045 in

- Relief Valve Spring Free Length

52.4 mm

2.06 in

Piston

- Clearance to Bore

0.025-0.045 mm

0.0010-0.0018 in

- Diameter

68.465-68.485 mm

2.695-2.696 in

Piston Pin

- Diameter

16.995-17.000 mm

0.6691-0.6693 in

- Pin Off-Set

0.4-06 mm

0.016-0.024 in

Piston Rings, End Gap

- Top Compression

0.15-0.30 mm

0.006-0.012 in

- 2nd Compression

0.30-0.45 mm

0.012-0.018 in

Piston Rings, Groove Clearance

- Top Impression

0.02-0.06 mm

0.0008-0.002 in

- 2nd Impression

0.02-0.06 mm

0.0008-0.002 in

Valve System

- Face Angle, All

45 degrees

- Face Runout, Maximum, All

0.045 mm

0.0018 in

- Seat Angle, All

45 degrees

- Seat Runout, Maximum, All

0.05 mm

0.0019 in

- Seat Width, Exhaust

1.56 mm

0.061 in

- Seat Width, Intake

1.56 mm

0.061 in

- Valve Diameter, All, Exhaust

31.7-31.9 mm

1.248-1.256 in

- Valve Diameter, All, Intake

35.5-35.7 mm

1.398-1.406 in

- Valve Guide Inside Diameter

5.500-5.512 mm

0.2165-0.2170 in

- Valve Lash Compensators

Mechanical

- Valve Spring Loads, Valve Closed

23.4-27 Kgf@44.2 mm

51.59-59.53 lbs@1.740 in

- Valve Spring Loads, Valve Open

51.7-58.3 Kgf@36.2 mm

113.97-128.53 lbs@1.425 in

- Valve Stem Diameter, Exhaust

5.440-5.455 mm

0.214-0.215 in

- Valve Stem Diameter, Intake

5.465-5.480 mm

0.215-0.216 in