For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Mounting Bracket Bolts | 30 N·m | 22.1 lb ft
Air Cleaner Assembly Bolts | 6 N·m | 4.4 lb ft
Air Filter Upper Housing Bolts | 2 N·m | 1.5 lb ft
Camshaft Cap Bolts | 10 N·m | 7.4 lb ft
Camshaft Sprocket Retaining Bolts | 60 N·m | 44.2 lb ft
Catalytic Converter Retaining Nuts | 40 N·m | 29.5 lb ft
Connecting Rod Bearing Cap Nuts | 33 N·m | 24.3 lb ft
Crankshaft Bearing Cap Bolts | 57.5 N·m | 42.4 lb ft
Crankshaft Pulley Bolt | 85 N·m | 62.7 lb ft
Crankshaft Rear Oil Seal Cover Bolts (M6 x 1.0) | 10.5 N·m | 7.7 lb ft
Cylinder Head Bolts | 22 + 82° N·m | 16.2 + 82° lb ft
Cylinder Head Cover Bolts | 10 N·m | 7.4 lb ft
Cylinder Head Cover Bracket Bolts | 10 N·m | 7.4 lb ft
Engine Mount Bracket Retaining Bolt/Nuts | 65 N·m | 47.9 lb ft
Engine Mount Retaining Bolts | 55 N·m | 40.5 lb ft
Exhaust Manifold Heat Shield Bolts | 15 N·m | 11 lb ft
Exhaust Manifold Retaining Bolts | 25 N·m | 18.4 lb ft
Exhaust Manifold Retaining Nuts | 20 N·m | 14.7 lb ft
Flywheel/Flexible Plate Bolts | 45 N·m | 33.2 lb ft
Front Exhaust Pipe-to-Front Muffler Nuts | 40 N·m | 29.5 lb ft
Front Exhaust Pipe-to-Main Catalytic Converter Nuts | 40 N·m | 29.5 lb ft
Generator Adjusting Bolt | 20 N·m | 14.7 lb ft
Generator Adjusting Bracket Retaining Bolt | 33 N·m | 24.3 lb ft
Intake Manifold Retaining Bolts | 10 N·m | 7.4 lb ft
Intake Manifold Support Bracket Upper Bolts | 2 N·m | 1.5 lb ft
Oil Level Gage Tube Retaining Bolt | 10.5 N·m | 7.7 lb ft
Oil Pan Retaining Bolts | 10.5 N·m | 7.7 lb ft
Oil Pressure Switch Fitting | 30 N·m | 22.1 lb ft
Oil Pump Cover Bolts | 10 N·m | 7.4 lb ft
Power Steering Pump Bracket Mounting Bolts | 20 N·m | 14.7 lb ft
Power Steering Pump Mounting Bolts | 20 N·m | 14.7 lb ft
Spark Plugs Cable Cover Bolts | 10 N·m | 7.4 lb ft
Timing Chain Cover Retaining Bolts (M6 x 1.0) | 10.5 N·m | 7.7 lb ft
Timing Chain Cover Retaining Bolts (M8 x 1.25) | 20 N·m | 14.7 lb ft
Timing Chain Guide Retaining Bolts | 10 N·m | 7.4 lb ft
Timing Chain Lever Retaining Bolts | 10 N·m | 7.4 lb ft
Timing Chain Tensioner Retaining Bolts | 12 N·m | 8.8 lb ft
Transmission Assembly Blots (M/T and A/T) | 60 N·m | 44.2 lb ft
Water Pump Retaining Bolts | 33 N·m | 24.3 lb ft