For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the floor console. Refer to Front Floor Console Replacement .
3. Disconnect the wiring harness connectors from the shift control lever.
4. Loosen the control cable adjusting nut.
5. Disconnect the control cable from the shift control lever assembly.
6. Remove the shift control lever assembly mounting bolts.
7. Remove the shift control lever assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the shift control lever assembly and mounting bolts.

Tighten
Tighten the shift control lever assembly mounting bolts to 8 N·m (71 lb in).

2. Connect the control cable to the shift control lever assembly.
3. Tighten the control cable adjusting nut.

Tighten
Tighten the control cable adjusting nut to 8 N·m (71 lb in).

4. Connect the harness connector.
5. Adjust the control cable. Refer to Range Selector Lever Cable Adjustment .
6. Install the floor console. Refer to Front Floor Console Replacement .
7. Connect the negative battery cable.