For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the sensor electrical connector.
3. Remove the camshaft position (CMP) sensor bolts and sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CMP sensor and bolts.

Tighten
Tighten the camshaft position bolts to 12 N·m (106 lb in).

2. Connect the sensor electrical connector.
3. Connect the negative battery cable.