For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Reposition the door seal trim.
3. Remove the bolts on the door and on the body.
4. Remove the door hold open link.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the door hold open link to the door and the body with the bolts.

Tighten

• | Tighten the door hold open link-to-body bolts to 35 N·m (26 lb ft).

• | Tighten the door hold open link-to-door bolts to 5 N·m (44 lb in).

2. Reposition the door seal trim.
3. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .