For 1990-2009 cars

### Removal Procedure

Notice: Refer to Brake Caliper Notice in the Preface section.

Important: To guarantee uniform braking on both sides, both rotors must have identical surfaces regarding smoothness and scoring depth. For this reason, always replace both rotors.

1. Remove the caliper assembly without disconnecting the brake hoses. Refer to Brake Caliper Replacement .
2. Remove the caliper bracket.
3. Remove the rotor-to-front wheel hub detent screw from the rotor and the front wheel hub.
4. Pull off the rotor.

### Installation Procedure

1. Inspect the rotor. Refer to Brake Rotor Surface and Wear Inspection .

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rotor to the front wheel hub by tightening the detent screw.

Tighten
Tighten the rotor-to-front wheel hub detent screw to 4 N·m (35 lb in).

3. Install the caliper bracket.

Tighten
Tighten the caliper bracket mounting bolts to 95 N·m (70 lb ft).

4. Install the caliper assembly. Refer to Brake Caliper Replacement .