For 1990-2009 cars

## Rear Side Door Sill Trim Plate Replacement Notchback

### Removal Procedure

1. Remove the rear seat cushion and the rear seatback. Refer to Rear Seat Cushion Replacement .
2. Remove the screw securing the rear rocker trim panel.
3. Pry off the rear rocker trim panel.

### Installation Procedure

1. Install the rear rocker trim panel.
2. Install the rear rocker trim panel with the screw.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear seat back with the bolt.

Tighten
Tighten the rear seatback bolt to 25 N·m (18 lb ft).

4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .

## Rear Side Door Sill Trim Plate Replacement Hatchback

### Removal Procedure

1. Remove the rear seat cushion and the rear seatback.

Refer to Rear Seat Cushion Replacement .

2. Remove the screw securing the rear rocker trim panel.
3. Pry off the rear rocker trim panel.

### Installation Procedure

1. Install the rear rocker trim panel.
2. Install the rear rocker trim panel with the screw.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear seatback with the bolt.

Tighten
Tighten the rear seatback bolt to 25 N·m (18 lb ft).

4. Install the rear seat cushion.

Refer to Rear Seat Cushion Replacement .