For 1990-2009 cars

### Removal Procedure

1. Disconnect the coolant heater power supply cord from the coolant heater (2).
2. Disconnect the coolant heater cord clip (1) from the engine lift bracket.
3. Disconnect the coolant heater cord from between the washer bottle and the coolant reservoir (1).
4. Remove the coolant heater cord from the vehicle.

### Installation Procedure

1. Connect the coolant heater cord to the coolant heater (2).
2. Secure the coolant heater cord clip (1) to the engine lift bracket.
3. Route the coolant heater cord along the battery (2).
4. Secure the coiled power cord between the washer fluid bottle and the coolant reservoir (1).