For 1990-2009 cars

### Removal Procedure

1. Remove the rear wheel speed sensor, if equipped. Refer to Rear Wheel Speed Sensor Replacement.
2. Remove the brake drum. Refer to Brake Drum Replacement.
3. Unstake the caulking nut (4).
4. Remove the caulking nut.

Important: Pull the wheel bearing and hub assembly straight off the spindle. The 2 inner wheel bearing races may not be secure.

5. Remove the wheel bearing and hub assembly (7) from the spindle (1).

### Installation Procedure

Important: Slide the wheel bearing and hub assembly straight onto the spindle. Use care in order to properly position the wheel bearing races on the spindle.

1. Install the wheel bearing and hub assembly (7) to the spindle (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the caulking nut (4) to the spindle.

Tighten
Tighten the nut to 190 N·m (140 lb ft).

3. Stake the caulking nut.
4. Install the brake drum. Refer to Brake Drum Replacement.
5. Install the rear wheel speed sensor, if equipped. Refer to Rear Wheel Speed Sensor Replacement.