For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the screws and the lower shield, if equipped.
3. Disconnect the speaker electrical connector.
4. Remove the door water deflector.

### Installation Procedure

1. Install the door water deflector.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door lower shield with the screws, if equipped.

Tighten
Tighten the door lower shield screws to 3.5 N·m (31 lb in).

3. Connect the speaker electrical connector.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .